<?xml version="1.0" encoding="utf-8"?>
<EduNetworkBuilder>
  <!--This is a network file for EduNetworkBuilder.-->
  <Network>
    <en_message>Both the switch and the firewall need VLANs set up on them for this puzzle to work.  You need to set them up from scratch.  Oh Joy. </en_message>
    <fr_message>Le commutateur et le pare-feu ont besoin que les VLAN soient configurés pour que le puzzle fonctionne. Vous devez les configurer à partir de zéro. Oh Joy.</fr_message>
    <en_title>NeedVLANs</en_title>
    <height>1024</height>
    <width>1024</width>
    <itemsize>100</itemsize>
    <showlabels>full</showlabels>
    <level>6</level>
    <sortorder>10</sortorder>
    <uniqueidentifier>148</uniqueidentifier>
    <startinghelplevel>full</startinghelplevel>
    <vlansenabled>True</vlansenabled>
    <VLANPacketColors>True</VLANPacketColors>
    <device>
      <hostname>firewall0</hostname>
      <size>100</size>
      <uniqueidentifier>142</uniqueidentifier>
      <location>390,170</location>
      <mytype>firewall</mytype>
      <isdns>False</isdns>
      <isdhcp>False</isdhcp>
      <hasadvfirewall>True</hasadvfirewall>
      <gateway>
        <ip>0.0.0.0</ip>
        <mask>0.0.0.0</mask>
        <gateway>0.0.0.0</gateway>
        <type>gw</type>
      </gateway>
      <nic>
        <nictype>lo</nictype>
        <nicname>lo0</nicname>
        <myid>
          <hostid>142</hostid>
          <nicid>143</nicid>
          <hostname>firewall0</hostname>
          <nicname>lo0</nicname>
        </myid>
        <nictype>lo</nictype>
        <uniqueidentifier>143</uniqueidentifier>
        <usesdhcp>False</usesdhcp>
        <interface>
          <nicname>lo0</nicname>
          <myip>
            <ip>127.0.0.1</ip>
            <mask>255.0.0.0</mask>
            <gateway>0.0.0.0</gateway>
            <type>ip</type>
          </myip>
          <VLAN
            ID="1">Untagged</VLAN>
        </interface>
      </nic>
      <nic>
        <nictype>wan</nictype>
        <nicname>wan0</nicname>
        <myid>
          <hostid>142</hostid>
          <nicid>146</nicid>
          <hostname>firewall0</hostname>
          <nicname>wan0</nicname>
        </myid>
        <nictype>wan</nictype>
        <uniqueidentifier>146</uniqueidentifier>
        <usesdhcp>False</usesdhcp>
        <interface>
          <nicname>wan0</nicname>
          <myip>
            <ip>0.0.0.0</ip>
            <mask>0.0.0.0</mask>
            <gateway>0.0.0.0</gateway>
            <type>ip</type>
          </myip>
          <VLAN
            ID="1">Untagged</VLAN>
        </interface>
      </nic>
      <nic>
        <nictype>eth</nictype>
        <nicname>eth0</nicname>
        <myid>
          <hostid>142</hostid>
          <nicid>144</nicid>
          <hostname>firewall0</hostname>
          <nicname>eth0</nicname>
        </myid>
        <nictype>eth</nictype>
        <uniqueidentifier>144</uniqueidentifier>
        <usesdhcp>False</usesdhcp>
        <interface>
          <nicname>eth0</nicname>
          <myip>
            <ip>192.168.1.1</ip>
            <mask>255.255.255.0</mask>
            <gateway>0.0.0.0</gateway>
            <type>ip</type>
          </myip>
          <VLAN
            ID="1">Untagged</VLAN>
        </interface>
        <interface>
          <nicname>eth0:1</nicname>
          <myip>
            <ip>192.168.2.1</ip>
            <mask>255.255.255.0</mask>
            <gateway>0.0.0.0</gateway>
            <type>ip</type>
          </myip>
          <VLAN
            ID="1">Untagged</VLAN>
          <VLAN
            ID="2">Forbidden</VLAN>
        </interface>
      </nic>
      <nic>
        <nictype>eth</nictype>
        <nicname>eth1</nicname>
        <myid>
          <hostid>142</hostid>
          <nicid>145</nicid>
          <hostname>firewall0</hostname>
          <nicname>eth1</nicname>
        </myid>
        <nictype>eth</nictype>
        <uniqueidentifier>145</uniqueidentifier>
        <usesdhcp>False</usesdhcp>
        <interface>
          <nicname>eth1</nicname>
          <myip>
            <ip>0.0.0.0</ip>
            <mask>0.0.0.0</mask>
            <gateway>0.0.0.0</gateway>
            <type>ip</type>
          </myip>
          <VLAN
            ID="1">Untagged</VLAN>
        </interface>
      </nic>
      <firwallrule>
        <source>eth0</source>
        <destination>eth0:1</destination>
        <action>Drop</action>
      </firwallrule>
      <firwallrule>
        <source>eth0:1</source>
        <destination>eth0</destination>
        <action>Drop</action>
      </firwallrule>
    </device>
    <device>
      <hostname>net_switch0</hostname>
      <size>100</size>
      <uniqueidentifier>109</uniqueidentifier>
      <location>390,400</location>
      <mytype>net_switch</mytype>
      <isdns>False</isdns>
      <isdhcp>False</isdhcp>
      <gateway>
        <ip>192.168.1.1</ip>
        <mask>0.0.0.0</mask>
        <gateway>0.0.0.0</gateway>
        <type>gw</type>
      </gateway>
      <nic>
        <nictype>lo</nictype>
        <nicname>lo0</nicname>
        <myid>
          <hostid>109</hostid>
          <nicid>110</nicid>
          <hostname>net_switch0</hostname>
          <nicname>lo0</nicname>
        </myid>
        <nictype>lo</nictype>
        <uniqueidentifier>110</uniqueidentifier>
        <usesdhcp>False</usesdhcp>
        <ssid />
        <interface>
          <nicname>lo0</nicname>
          <myip>
            <ip>127.0.0.1</ip>
            <mask>255.0.0.0</mask>
            <gateway>0.0.0.0</gateway>
            <type>ip</type>
          </myip>
          <VLAN
            ID="1">Untagged</VLAN>
        </interface>
      </nic>
      <nic>
        <nictype>management_interface</nictype>
        <nicname>management_interface0</nicname>
        <myid>
          <hostid>109</hostid>
          <nicid>111</nicid>
          <hostname>net_switch0</hostname>
          <nicname>management_interface0</nicname>
        </myid>
        <nictype>management_interface</nictype>
        <uniqueidentifier>111</uniqueidentifier>
        <usesdhcp>False</usesdhcp>
        <ssid />
        <interface>
          <nicname>management_interface0</nicname>
          <myip>
            <ip>192.168.1.5</ip>
            <mask>255.255.255.0</mask>
            <gateway>0.0.0.0</gateway>
            <type>ip</type>
          </myip>
          <VLAN
            ID="1">Untagged</VLAN>
        </interface>
      </nic>
      <nic>
        <nictype>port</nictype>
        <nicname>port1</nicname>
        <myid>
          <hostid>109</hostid>
          <nicid>112</nicid>
          <hostname>net_switch0</hostname>
          <nicname>port1</nicname>
        </myid>
        <nictype>port</nictype>
        <uniqueidentifier>112</uniqueidentifier>
        <usesdhcp>False</usesdhcp>
        <ssid />
        <interface>
          <nicname>port1</nicname>
          <myip>
            <ip>0.0.0.0</ip>
            <mask>0.0.0.0</mask>
            <gateway>0.0.0.0</gateway>
            <type>ip</type>
          </myip>
          <VLAN
            ID="1">Untagged</VLAN>
          <VLAN
            ID="2">Forbidden</VLAN>
        </interface>
      </nic>
      <nic>
        <nictype>port</nictype>
        <nicname>port2</nicname>
        <myid>
          <hostid>109</hostid>
          <nicid>113</nicid>
          <hostname>net_switch0</hostname>
          <nicname>port2</nicname>
        </myid>
        <nictype>port</nictype>
        <uniqueidentifier>113</uniqueidentifier>
        <usesdhcp>False</usesdhcp>
        <ssid />
        <interface>
          <nicname>port2</nicname>
          <myip>
            <ip>0.0.0.0</ip>
            <mask>0.0.0.0</mask>
            <gateway>0.0.0.0</gateway>
            <type>ip</type>
          </myip>
          <VLAN
            ID="1">Untagged</VLAN>
          <VLAN
            ID="2">Forbidden</VLAN>
        </interface>
      </nic>
      <nic>
        <nictype>port</nictype>
        <nicname>port3</nicname>
        <myid>
          <hostid>109</hostid>
          <nicid>114</nicid>
          <hostname>net_switch0</hostname>
          <nicname>port3</nicname>
        </myid>
        <nictype>port</nictype>
        <uniqueidentifier>114</uniqueidentifier>
        <usesdhcp>False</usesdhcp>
        <ssid />
        <interface>
          <nicname>port3</nicname>
          <myip>
            <ip>0.0.0.0</ip>
            <mask>0.0.0.0</mask>
            <gateway>0.0.0.0</gateway>
            <type>ip</type>
          </myip>
          <VLAN
            ID="1">Untagged</VLAN>
          <VLAN
            ID="2">Forbidden</VLAN>
        </interface>
      </nic>
      <nic>
        <nictype>port</nictype>
        <nicname>port4</nicname>
        <myid>
          <hostid>109</hostid>
          <nicid>115</nicid>
          <hostname>net_switch0</hostname>
          <nicname>port4</nicname>
        </myid>
        <nictype>port</nictype>
        <uniqueidentifier>115</uniqueidentifier>
        <usesdhcp>False</usesdhcp>
        <ssid />
        <interface>
          <nicname>port4</nicname>
          <myip>
            <ip>0.0.0.0</ip>
            <mask>0.0.0.0</mask>
            <gateway>0.0.0.0</gateway>
            <type>ip</type>
          </myip>
          <VLAN
            ID="1">Untagged</VLAN>
          <VLAN
            ID="2">Forbidden</VLAN>
        </interface>
      </nic>
      <nic>
        <nictype>port</nictype>
        <nicname>port5</nicname>
        <myid>
          <hostid>109</hostid>
          <nicid>116</nicid>
          <hostname>net_switch0</hostname>
          <nicname>port5</nicname>
        </myid>
        <nictype>port</nictype>
        <uniqueidentifier>116</uniqueidentifier>
        <usesdhcp>False</usesdhcp>
        <ssid />
        <interface>
          <nicname>port5</nicname>
          <myip>
            <ip>0.0.0.0</ip>
            <mask>0.0.0.0</mask>
            <gateway>0.0.0.0</gateway>
            <type>ip</type>
          </myip>
          <VLAN
            ID="1">Untagged</VLAN>
          <VLAN
            ID="2">Forbidden</VLAN>
        </interface>
      </nic>
      <nic>
        <nictype>port</nictype>
        <nicname>port6</nicname>
        <myid>
          <hostid>109</hostid>
          <nicid>117</nicid>
          <hostname>net_switch0</hostname>
          <nicname>port6</nicname>
        </myid>
        <nictype>port</nictype>
        <uniqueidentifier>117</uniqueidentifier>
        <usesdhcp>False</usesdhcp>
        <ssid />
        <interface>
          <nicname>port6</nicname>
          <myip>
            <ip>0.0.0.0</ip>
            <mask>0.0.0.0</mask>
            <gateway>0.0.0.0</gateway>
            <type>ip</type>
          </myip>
          <VLAN
            ID="1">Untagged</VLAN>
          <VLAN
            ID="2">Forbidden</VLAN>
        </interface>
      </nic>
      <nic>
        <nictype>port</nictype>
        <nicname>port7</nicname>
        <myid>
          <hostid>109</hostid>
          <nicid>118</nicid>
          <hostname>net_switch0</hostname>
          <nicname>port7</nicname>
        </myid>
        <nictype>port</nictype>
        <uniqueidentifier>118</uniqueidentifier>
        <usesdhcp>False</usesdhcp>
        <ssid />
        <interface>
          <nicname>port7</nicname>
          <myip>
            <ip>0.0.0.0</ip>
            <mask>0.0.0.0</mask>
            <gateway>0.0.0.0</gateway>
            <type>ip</type>
          </myip>
          <VLAN
            ID="1">Untagged</VLAN>
          <VLAN
            ID="2">Forbidden</VLAN>
        </interface>
      </nic>
    </device>
    <device>
      <hostname>pc0</hostname>
      <size>100</size>
      <uniqueidentifier>121</uniqueidentifier>
      <location>80,490</location>
      <mytype>pc</mytype>
      <isdns>False</isdns>
      <isdhcp>False</isdhcp>
      <morphcolor>Pink</morphcolor>
      <gateway>
        <ip>192.168.1.1</ip>
        <mask>0.0.0.0</mask>
        <gateway>0.0.0.0</gateway>
        <type>gw</type>
      </gateway>
      <nic>
        <nictype>lo</nictype>
        <nicname>lo0</nicname>
        <myid>
          <hostid>121</hostid>
          <nicid>122</nicid>
          <hostname>pc0</hostname>
          <nicname>lo0</nicname>
        </myid>
        <nictype>lo</nictype>
        <uniqueidentifier>122</uniqueidentifier>
        <usesdhcp>False</usesdhcp>
        <ssid />
        <interface>
          <nicname>lo0</nicname>
          <myip>
            <ip>127.0.0.1</ip>
            <mask>255.0.0.0</mask>
            <gateway>0.0.0.0</gateway>
            <type>ip</type>
          </myip>
          <VLAN
            ID="1">Untagged</VLAN>
        </interface>
      </nic>
      <nic>
        <nictype>eth</nictype>
        <nicname>eth0</nicname>
        <myid>
          <hostid>121</hostid>
          <nicid>123</nicid>
          <hostname>pc0</hostname>
          <nicname>eth0</nicname>
        </myid>
        <nictype>eth</nictype>
        <uniqueidentifier>123</uniqueidentifier>
        <usesdhcp>False</usesdhcp>
        <ssid />
        <interface>
          <nicname>eth0</nicname>
          <myip>
            <ip>192.168.1.2</ip>
            <mask>255.255.255.0</mask>
            <gateway>0.0.0.0</gateway>
            <type>ip</type>
          </myip>
          <VLAN
            ID="1">Untagged</VLAN>
        </interface>
      </nic>
    </device>
    <device>
      <hostname>pc1</hostname>
      <size>100</size>
      <uniqueidentifier>124</uniqueidentifier>
      <location>90,820</location>
      <mytype>pc</mytype>
      <isdns>False</isdns>
      <isdhcp>False</isdhcp>
      <morphcolor>Pink</morphcolor>
      <gateway>
        <ip>192.168.1.1</ip>
        <mask>0.0.0.0</mask>
        <gateway>0.0.0.0</gateway>
        <type>gw</type>
      </gateway>
      <nic>
        <nictype>lo</nictype>
        <nicname>lo0</nicname>
        <myid>
          <hostid>124</hostid>
          <nicid>125</nicid>
          <hostname>pc1</hostname>
          <nicname>lo0</nicname>
        </myid>
        <nictype>lo</nictype>
        <uniqueidentifier>125</uniqueidentifier>
        <usesdhcp>False</usesdhcp>
        <ssid />
        <interface>
          <nicname>lo0</nicname>
          <myip>
            <ip>127.0.0.1</ip>
            <mask>255.0.0.0</mask>
            <gateway>0.0.0.0</gateway>
            <type>ip</type>
          </myip>
          <VLAN
            ID="1">Untagged</VLAN>
        </interface>
      </nic>
      <nic>
        <nictype>eth</nictype>
        <nicname>eth0</nicname>
        <myid>
          <hostid>124</hostid>
          <nicid>126</nicid>
          <hostname>pc1</hostname>
          <nicname>eth0</nicname>
        </myid>
        <nictype>eth</nictype>
        <uniqueidentifier>126</uniqueidentifier>
        <usesdhcp>False</usesdhcp>
        <ssid />
        <interface>
          <nicname>eth0</nicname>
          <myip>
            <ip>192.168.1.3</ip>
            <mask>255.255.255.0</mask>
            <gateway>0.0.0.0</gateway>
            <type>ip</type>
          </myip>
          <VLAN
            ID="1">Untagged</VLAN>
        </interface>
      </nic>
    </device>
    <device>
      <hostname>pc2</hostname>
      <size>100</size>
      <uniqueidentifier>127</uniqueidentifier>
      <location>710,820</location>
      <mytype>pc</mytype>
      <isdns>False</isdns>
      <isdhcp>False</isdhcp>
      <morphcolor>LightBlue</morphcolor>
      <gateway>
        <ip>192.168.2.1</ip>
        <mask>0.0.0.0</mask>
        <gateway>0.0.0.0</gateway>
        <type>gw</type>
      </gateway>
      <nic>
        <nictype>lo</nictype>
        <nicname>lo0</nicname>
        <myid>
          <hostid>127</hostid>
          <nicid>128</nicid>
          <hostname>pc2</hostname>
          <nicname>lo0</nicname>
        </myid>
        <nictype>lo</nictype>
        <uniqueidentifier>128</uniqueidentifier>
        <usesdhcp>False</usesdhcp>
        <ssid />
        <interface>
          <nicname>lo0</nicname>
          <myip>
            <ip>127.0.0.1</ip>
            <mask>255.0.0.0</mask>
            <gateway>0.0.0.0</gateway>
            <type>ip</type>
          </myip>
          <VLAN
            ID="1">Untagged</VLAN>
        </interface>
      </nic>
      <nic>
        <nictype>eth</nictype>
        <nicname>eth0</nicname>
        <myid>
          <hostid>127</hostid>
          <nicid>129</nicid>
          <hostname>pc2</hostname>
          <nicname>eth0</nicname>
        </myid>
        <nictype>eth</nictype>
        <uniqueidentifier>129</uniqueidentifier>
        <usesdhcp>False</usesdhcp>
        <ssid />
        <interface>
          <nicname>eth0</nicname>
          <myip>
            <ip>192.168.2.3</ip>
            <mask>255.255.255.0</mask>
            <gateway>0.0.0.0</gateway>
            <type>ip</type>
          </myip>
          <VLAN
            ID="1">Untagged</VLAN>
        </interface>
      </nic>
    </device>
    <device>
      <hostname>pc3</hostname>
      <size>100</size>
      <uniqueidentifier>130</uniqueidentifier>
      <location>760,500</location>
      <mytype>pc</mytype>
      <isdns>False</isdns>
      <isdhcp>False</isdhcp>
      <morphcolor>LightBlue</morphcolor>
      <gateway>
        <ip>192.168.2.1</ip>
        <mask>0.0.0.0</mask>
        <gateway>0.0.0.0</gateway>
        <type>gw</type>
      </gateway>
      <nic>
        <nictype>lo</nictype>
        <nicname>lo0</nicname>
        <myid>
          <hostid>130</hostid>
          <nicid>131</nicid>
          <hostname>pc3</hostname>
          <nicname>lo0</nicname>
        </myid>
        <nictype>lo</nictype>
        <uniqueidentifier>131</uniqueidentifier>
        <usesdhcp>False</usesdhcp>
        <ssid />
        <interface>
          <nicname>lo0</nicname>
          <myip>
            <ip>127.0.0.1</ip>
            <mask>255.0.0.0</mask>
            <gateway>0.0.0.0</gateway>
            <type>ip</type>
          </myip>
          <VLAN
            ID="1">Untagged</VLAN>
        </interface>
      </nic>
      <nic>
        <nictype>eth</nictype>
        <nicname>eth0</nicname>
        <myid>
          <hostid>130</hostid>
          <nicid>132</nicid>
          <hostname>pc3</hostname>
          <nicname>eth0</nicname>
        </myid>
        <nictype>eth</nictype>
        <uniqueidentifier>132</uniqueidentifier>
        <usesdhcp>False</usesdhcp>
        <ssid />
        <interface>
          <nicname>eth0</nicname>
          <myip>
            <ip>192.168.2.2</ip>
            <mask>255.255.255.0</mask>
            <gateway>0.0.0.0</gateway>
            <type>ip</type>
          </myip>
          <VLAN
            ID="1">Untagged</VLAN>
        </interface>
      </nic>
    </device>
    <link>
      <SrcNic>
        <hostid>121</hostid>
        <nicid>123</nicid>
        <hostname>pc0</hostname>
        <nicname>eth0</nicname>
      </SrcNic>
      <DstNic>
        <hostid>109</hostid>
        <nicid>114</nicid>
        <hostname>net_switch0</hostname>
        <nicname>port3</nicname>
      </DstNic>
      <hostname>pc0_link_net_switch0</hostname>
      <linktype>normal</linktype>
      <uniqueidentifier>133</uniqueidentifier>
    </link>
    <link>
      <SrcNic>
        <hostid>124</hostid>
        <nicid>126</nicid>
        <hostname>pc1</hostname>
        <nicname>eth0</nicname>
      </SrcNic>
      <DstNic>
        <hostid>109</hostid>
        <nicid>115</nicid>
        <hostname>net_switch0</hostname>
        <nicname>port4</nicname>
      </DstNic>
      <hostname>pc1_link_net_switch0</hostname>
      <linktype>normal</linktype>
      <uniqueidentifier>134</uniqueidentifier>
    </link>
    <link>
      <SrcNic>
        <hostid>127</hostid>
        <nicid>129</nicid>
        <hostname>pc2</hostname>
        <nicname>eth0</nicname>
      </SrcNic>
      <DstNic>
        <hostid>109</hostid>
        <nicid>116</nicid>
        <hostname>net_switch0</hostname>
        <nicname>port5</nicname>
      </DstNic>
      <hostname>pc2_link_net_switch0</hostname>
      <linktype>normal</linktype>
      <uniqueidentifier>135</uniqueidentifier>
    </link>
    <link>
      <SrcNic>
        <hostid>130</hostid>
        <nicid>132</nicid>
        <hostname>pc3</hostname>
        <nicname>eth0</nicname>
      </SrcNic>
      <DstNic>
        <hostid>109</hostid>
        <nicid>117</nicid>
        <hostname>net_switch0</hostname>
        <nicname>port6</nicname>
      </DstNic>
      <hostname>pc3_link_net_switch0</hostname>
      <linktype>normal</linktype>
      <uniqueidentifier>136</uniqueidentifier>
    </link>
    <link>
      <SrcNic>
        <hostid>109</hostid>
        <nicid>118</nicid>
        <hostname>net_switch0</hostname>
        <nicname>port7</nicname>
      </SrcNic>
      <DstNic>
        <hostid>142</hostid>
        <nicid>144</nicid>
        <hostname>firewall0</hostname>
        <nicname>eth0</nicname>
      </DstNic>
      <hostname>net_switch0_link_firewall0</hostname>
      <linktype>normal</linktype>
      <uniqueidentifier>147</uniqueidentifier>
    </link>
    <nettest>
      <shost>pc0</shost>
      <dhost>pc1</dhost>
      <thetest>SuccessfullyPings</thetest>
    </nettest>
    <nettest>
      <shost>pc0</shost>
      <dhost>pc2</dhost>
      <thetest>SuccessfullyPings</thetest>
    </nettest>
    <nettest>
      <shost>pc3</shost>
      <dhost>pc1</dhost>
      <thetest>SuccessfullyPings</thetest>
    </nettest>
    <nettest>
      <shost>pc3</shost>
      <dhost>pc2</dhost>
      <thetest>SuccessfullyPings</thetest>
    </nettest>
    <nettest>
      <shost>pc0</shost>
      <dhost>192.168.1.255</dhost>
      <thetest>SuccessfullyPings</thetest>
    </nettest>
    <nettest>
      <shost>pc3</shost>
      <dhost>192.168.2.255</dhost>
      <thetest>SuccessfullyPings</thetest>
    </nettest>
    <tag>Subnet</tag>
    <tag>Ping</tag>
    <tag>Router</tag>
    <tag>VLAN</tag>
    <VLANName
      ID="1"
      Color="Purple">Default</VLANName>
    <VLANName
      ID="2"
      Color="Cyan">Staff</VLANName>
  </Network>
</EduNetworkBuilder>