<?xml version="1.0" encoding="utf-8"?>
<EduNetworkBuilder>
  <!--This is a network file for EduNetworkBuilder.-->
  <Network>
    <en_message>Firewall devices can have an advanced firewall.  You can control which interfaces can ping which interfaces.  This allows you to protect one side of the LAN from the other.  We will use this functionality a lot more later on.
This technology is mainly used for VLAN security, or setting up a DMZ.  To do this puzzle, remove the firewall rule that is keeping the one side from pinging the other side.</en_message>
    <fr_message>Les pare-feu peuvent avoir un pare-feu avancé. Vous pouvez contrôler quelles interfaces peuvent cingler quelles interfaces. Cela vous permet de protéger un côté du réseau local de l'autre. Nous utiliserons cette fonctionnalité beaucoup plus tard.
Cette technologie est principalement utilisée pour la sécurité VLAN, ou la mise en place d'une DMZ. Pour ce casse-tête, supprimez la règle du pare-feu qui empêche le côté d'envoyer un ping de l'autre côté.</fr_message>
    <en_title>Firewall Test 2</en_title>
    <height>1024</height>
    <width>1024</width>
    <itemsize>100</itemsize>
    <showlabels>none</showlabels>
    <level>2</level>
    <sortorder>0.01</sortorder>
    <uniqueidentifier>158</uniqueidentifier>
    <startinghelplevel>full</startinghelplevel>
    <vlansenabled>True</vlansenabled>
    <VLANPacketColors>False</VLANPacketColors>
    <device>
      <hostname>firewall0</hostname>
      <size>100</size>
      <uniqueidentifier>100</uniqueidentifier>
      <location>410,410</location>
      <mytype>firewall</mytype>
      <isdns>False</isdns>
      <isdhcp>True</isdhcp>
      <hasadvfirewall>True</hasadvfirewall>
      <gateway>
        <ip>192.168.1.1</ip>
        <mask>0.0.0.0</mask>
        <gateway>0.0.0.0</gateway>
        <type>gw</type>
      </gateway>
      <nic>
        <nictype>wan</nictype>
        <nicname>wan0</nicname>
        <myid>
          <hostid>100</hostid>
          <nicid>104</nicid>
          <hostname>firewall0</hostname>
          <nicname>wan0</nicname>
        </myid>
        <nictype>wan</nictype>
        <uniqueidentifier>104</uniqueidentifier>
        <usesdhcp>False</usesdhcp>
        <encryptionkey />
        <interface>
          <nicname>wan0</nicname>
          <myip>
            <ip>192.168.5.1</ip>
            <mask>255.255.255.0</mask>
            <gateway>0.0.0.0</gateway>
            <type>ip</type>
          </myip>
          <VLAN
            ID="1">Untagged</VLAN>
        </interface>
      </nic>
      <nic>
        <nictype>lo</nictype>
        <nicname>lo0</nicname>
        <myid>
          <hostid>100</hostid>
          <nicid>101</nicid>
          <hostname>firewall0</hostname>
          <nicname>lo0</nicname>
        </myid>
        <nictype>lo</nictype>
        <uniqueidentifier>101</uniqueidentifier>
        <usesdhcp>False</usesdhcp>
        <encryptionkey />
        <interface>
          <nicname>lo0</nicname>
          <myip>
            <ip>127.0.0.1</ip>
            <mask>255.0.0.0</mask>
            <gateway>0.0.0.0</gateway>
            <type>ip</type>
          </myip>
          <VLAN
            ID="1">Untagged</VLAN>
        </interface>
      </nic>
      <nic>
        <nictype>eth</nictype>
        <nicname>eth0</nicname>
        <myid>
          <hostid>100</hostid>
          <nicid>102</nicid>
          <hostname>firewall0</hostname>
          <nicname>eth0</nicname>
        </myid>
        <nictype>eth</nictype>
        <uniqueidentifier>102</uniqueidentifier>
        <usesdhcp>False</usesdhcp>
        <encryptionkey />
        <interface>
          <nicname>eth0</nicname>
          <myip>
            <ip>192.168.1.1</ip>
            <mask>255.255.255.0</mask>
            <gateway>0.0.0.0</gateway>
            <type>ip</type>
          </myip>
          <VLAN
            ID="1">Untagged</VLAN>
        </interface>
      </nic>
      <nic>
        <nictype>eth</nictype>
        <nicname>eth1</nicname>
        <myid>
          <hostid>100</hostid>
          <nicid>103</nicid>
          <hostname>firewall0</hostname>
          <nicname>eth1</nicname>
        </myid>
        <nictype>eth</nictype>
        <uniqueidentifier>103</uniqueidentifier>
        <usesdhcp>False</usesdhcp>
        <encryptionkey />
        <interface>
          <nicname>eth1</nicname>
          <myip>
            <ip>192.168.2.1</ip>
            <mask>255.255.255.0</mask>
            <gateway>0.0.0.0</gateway>
            <type>ip</type>
          </myip>
          <VLAN
            ID="1">Untagged</VLAN>
        </interface>
      </nic>
      <dhcprange>
        <ip>192.168.5.1</ip>
        <mask>0.0.0.0</mask>
        <gateway>0.0.0.0</gateway>
        <type>route</type>
      </dhcprange>
      <dhcprange>
        <ip>127.0.0.1</ip>
        <mask>0.0.0.0</mask>
        <gateway>0.0.0.0</gateway>
        <type>route</type>
      </dhcprange>
      <dhcprange>
        <ip>192.168.1.1</ip>
        <mask>192.168.1.5</mask>
        <gateway>192.168.1.10</gateway>
        <type>route</type>
      </dhcprange>
      <dhcprange>
        <ip>192.168.2.1</ip>
        <mask>192.168.2.5</mask>
        <gateway>192.168.2.10</gateway>
        <type>route</type>
      </dhcprange>
      <firwallrule>
        <source>eth0</source>
        <destination>eth1</destination>
        <action>Drop</action>
      </firwallrule>
    </device>
    <device>
      <hostname>net_switch0</hostname>
      <size>100</size>
      <uniqueidentifier>105</uniqueidentifier>
      <location>410,190</location>
      <mytype>net_switch</mytype>
      <isdns>False</isdns>
      <isdhcp>False</isdhcp>
      <gateway>
        <ip>0.0.0.0</ip>
        <mask>0.0.0.0</mask>
        <gateway>0.0.0.0</gateway>
        <type>gw</type>
      </gateway>
      <nic>
        <nictype>lo</nictype>
        <nicname>lo0</nicname>
        <myid>
          <hostid>105</hostid>
          <nicid>106</nicid>
          <hostname>net_switch0</hostname>
          <nicname>lo0</nicname>
        </myid>
        <nictype>lo</nictype>
        <uniqueidentifier>106</uniqueidentifier>
        <usesdhcp>False</usesdhcp>
        <encryptionkey />
        <interface>
          <nicname>lo0</nicname>
          <myip>
            <ip>127.0.0.1</ip>
            <mask>255.0.0.0</mask>
            <gateway>0.0.0.0</gateway>
            <type>ip</type>
          </myip>
          <VLAN
            ID="1">Untagged</VLAN>
        </interface>
      </nic>
      <nic>
        <nictype>management_interface</nictype>
        <nicname>management_interface0</nicname>
        <myid>
          <hostid>105</hostid>
          <nicid>107</nicid>
          <hostname>net_switch0</hostname>
          <nicname>management_interface0</nicname>
        </myid>
        <nictype>management_interface</nictype>
        <uniqueidentifier>107</uniqueidentifier>
        <usesdhcp>False</usesdhcp>
        <encryptionkey />
        <interface>
          <nicname>management_interface0</nicname>
          <myip>
            <ip>0.0.0.0</ip>
            <mask>0.0.0.0</mask>
            <gateway>0.0.0.0</gateway>
            <type>ip</type>
          </myip>
          <VLAN
            ID="1">Untagged</VLAN>
        </interface>
      </nic>
      <nic>
        <nictype>port</nictype>
        <nicname>port1</nicname>
        <myid>
          <hostid>105</hostid>
          <nicid>108</nicid>
          <hostname>net_switch0</hostname>
          <nicname>port1</nicname>
        </myid>
        <nictype>port</nictype>
        <uniqueidentifier>108</uniqueidentifier>
        <usesdhcp>False</usesdhcp>
        <encryptionkey />
        <interface>
          <nicname>port1</nicname>
          <myip>
            <ip>0.0.0.0</ip>
            <mask>0.0.0.0</mask>
            <gateway>0.0.0.0</gateway>
            <type>ip</type>
          </myip>
          <VLAN
            ID="1">Untagged</VLAN>
        </interface>
      </nic>
      <nic>
        <nictype>port</nictype>
        <nicname>port2</nicname>
        <myid>
          <hostid>105</hostid>
          <nicid>109</nicid>
          <hostname>net_switch0</hostname>
          <nicname>port2</nicname>
        </myid>
        <nictype>port</nictype>
        <uniqueidentifier>109</uniqueidentifier>
        <usesdhcp>False</usesdhcp>
        <encryptionkey />
        <interface>
          <nicname>port2</nicname>
          <myip>
            <ip>0.0.0.0</ip>
            <mask>0.0.0.0</mask>
            <gateway>0.0.0.0</gateway>
            <type>ip</type>
          </myip>
          <VLAN
            ID="1">Untagged</VLAN>
        </interface>
      </nic>
      <nic>
        <nictype>port</nictype>
        <nicname>port3</nicname>
        <myid>
          <hostid>105</hostid>
          <nicid>110</nicid>
          <hostname>net_switch0</hostname>
          <nicname>port3</nicname>
        </myid>
        <nictype>port</nictype>
        <uniqueidentifier>110</uniqueidentifier>
        <usesdhcp>False</usesdhcp>
        <encryptionkey />
        <interface>
          <nicname>port3</nicname>
          <myip>
            <ip>0.0.0.0</ip>
            <mask>0.0.0.0</mask>
            <gateway>0.0.0.0</gateway>
            <type>ip</type>
          </myip>
          <VLAN
            ID="1">Untagged</VLAN>
        </interface>
      </nic>
      <nic>
        <nictype>port</nictype>
        <nicname>port4</nicname>
        <myid>
          <hostid>105</hostid>
          <nicid>111</nicid>
          <hostname>net_switch0</hostname>
          <nicname>port4</nicname>
        </myid>
        <nictype>port</nictype>
        <uniqueidentifier>111</uniqueidentifier>
        <usesdhcp>False</usesdhcp>
        <encryptionkey />
        <interface>
          <nicname>port4</nicname>
          <myip>
            <ip>0.0.0.0</ip>
            <mask>0.0.0.0</mask>
            <gateway>0.0.0.0</gateway>
            <type>ip</type>
          </myip>
          <VLAN
            ID="1">Untagged</VLAN>
        </interface>
      </nic>
      <nic>
        <nictype>port</nictype>
        <nicname>port5</nicname>
        <myid>
          <hostid>105</hostid>
          <nicid>112</nicid>
          <hostname>net_switch0</hostname>
          <nicname>port5</nicname>
        </myid>
        <nictype>port</nictype>
        <uniqueidentifier>112</uniqueidentifier>
        <usesdhcp>False</usesdhcp>
        <encryptionkey />
        <interface>
          <nicname>port5</nicname>
          <myip>
            <ip>0.0.0.0</ip>
            <mask>0.0.0.0</mask>
            <gateway>0.0.0.0</gateway>
            <type>ip</type>
          </myip>
          <VLAN
            ID="1">Untagged</VLAN>
        </interface>
      </nic>
      <nic>
        <nictype>port</nictype>
        <nicname>port6</nicname>
        <myid>
          <hostid>105</hostid>
          <nicid>113</nicid>
          <hostname>net_switch0</hostname>
          <nicname>port6</nicname>
        </myid>
        <nictype>port</nictype>
        <uniqueidentifier>113</uniqueidentifier>
        <usesdhcp>False</usesdhcp>
        <encryptionkey />
        <interface>
          <nicname>port6</nicname>
          <myip>
            <ip>0.0.0.0</ip>
            <mask>0.0.0.0</mask>
            <gateway>0.0.0.0</gateway>
            <type>ip</type>
          </myip>
          <VLAN
            ID="1">Untagged</VLAN>
        </interface>
      </nic>
      <nic>
        <nictype>port</nictype>
        <nicname>port7</nicname>
        <myid>
          <hostid>105</hostid>
          <nicid>114</nicid>
          <hostname>net_switch0</hostname>
          <nicname>port7</nicname>
        </myid>
        <nictype>port</nictype>
        <uniqueidentifier>114</uniqueidentifier>
        <usesdhcp>False</usesdhcp>
        <encryptionkey />
        <interface>
          <nicname>port7</nicname>
          <myip>
            <ip>0.0.0.0</ip>
            <mask>0.0.0.0</mask>
            <gateway>0.0.0.0</gateway>
            <type>ip</type>
          </myip>
          <VLAN
            ID="1">Untagged</VLAN>
        </interface>
      </nic>
    </device>
    <device>
      <hostname>net_switch1</hostname>
      <size>100</size>
      <uniqueidentifier>118</uniqueidentifier>
      <location>230,410</location>
      <mytype>net_switch</mytype>
      <isdns>False</isdns>
      <isdhcp>False</isdhcp>
      <gateway>
        <ip>0.0.0.0</ip>
        <mask>0.0.0.0</mask>
        <gateway>0.0.0.0</gateway>
        <type>gw</type>
      </gateway>
      <nic>
        <nictype>lo</nictype>
        <nicname>lo0</nicname>
        <myid>
          <hostid>118</hostid>
          <nicid>119</nicid>
          <hostname>net_switch1</hostname>
          <nicname>lo0</nicname>
        </myid>
        <nictype>lo</nictype>
        <uniqueidentifier>119</uniqueidentifier>
        <usesdhcp>False</usesdhcp>
        <encryptionkey />
        <interface>
          <nicname>lo0</nicname>
          <myip>
            <ip>127.0.0.1</ip>
            <mask>255.0.0.0</mask>
            <gateway>0.0.0.0</gateway>
            <type>ip</type>
          </myip>
          <VLAN
            ID="1">Untagged</VLAN>
        </interface>
      </nic>
      <nic>
        <nictype>management_interface</nictype>
        <nicname>management_interface0</nicname>
        <myid>
          <hostid>118</hostid>
          <nicid>120</nicid>
          <hostname>net_switch1</hostname>
          <nicname>management_interface0</nicname>
        </myid>
        <nictype>management_interface</nictype>
        <uniqueidentifier>120</uniqueidentifier>
        <usesdhcp>False</usesdhcp>
        <encryptionkey />
        <interface>
          <nicname>management_interface0</nicname>
          <myip>
            <ip>0.0.0.0</ip>
            <mask>0.0.0.0</mask>
            <gateway>0.0.0.0</gateway>
            <type>ip</type>
          </myip>
          <VLAN
            ID="1">Untagged</VLAN>
        </interface>
      </nic>
      <nic>
        <nictype>port</nictype>
        <nicname>port1</nicname>
        <myid>
          <hostid>118</hostid>
          <nicid>121</nicid>
          <hostname>net_switch1</hostname>
          <nicname>port1</nicname>
        </myid>
        <nictype>port</nictype>
        <uniqueidentifier>121</uniqueidentifier>
        <usesdhcp>False</usesdhcp>
        <encryptionkey />
        <interface>
          <nicname>port1</nicname>
          <myip>
            <ip>0.0.0.0</ip>
            <mask>0.0.0.0</mask>
            <gateway>0.0.0.0</gateway>
            <type>ip</type>
          </myip>
          <VLAN
            ID="1">Untagged</VLAN>
        </interface>
      </nic>
      <nic>
        <nictype>port</nictype>
        <nicname>port2</nicname>
        <myid>
          <hostid>118</hostid>
          <nicid>122</nicid>
          <hostname>net_switch1</hostname>
          <nicname>port2</nicname>
        </myid>
        <nictype>port</nictype>
        <uniqueidentifier>122</uniqueidentifier>
        <usesdhcp>False</usesdhcp>
        <encryptionkey />
        <interface>
          <nicname>port2</nicname>
          <myip>
            <ip>0.0.0.0</ip>
            <mask>0.0.0.0</mask>
            <gateway>0.0.0.0</gateway>
            <type>ip</type>
          </myip>
          <VLAN
            ID="1">Untagged</VLAN>
        </interface>
      </nic>
      <nic>
        <nictype>port</nictype>
        <nicname>port3</nicname>
        <myid>
          <hostid>118</hostid>
          <nicid>123</nicid>
          <hostname>net_switch1</hostname>
          <nicname>port3</nicname>
        </myid>
        <nictype>port</nictype>
        <uniqueidentifier>123</uniqueidentifier>
        <usesdhcp>False</usesdhcp>
        <encryptionkey />
        <interface>
          <nicname>port3</nicname>
          <myip>
            <ip>0.0.0.0</ip>
            <mask>0.0.0.0</mask>
            <gateway>0.0.0.0</gateway>
            <type>ip</type>
          </myip>
          <VLAN
            ID="1">Untagged</VLAN>
        </interface>
      </nic>
      <nic>
        <nictype>port</nictype>
        <nicname>port4</nicname>
        <myid>
          <hostid>118</hostid>
          <nicid>124</nicid>
          <hostname>net_switch1</hostname>
          <nicname>port4</nicname>
        </myid>
        <nictype>port</nictype>
        <uniqueidentifier>124</uniqueidentifier>
        <usesdhcp>False</usesdhcp>
        <encryptionkey />
        <interface>
          <nicname>port4</nicname>
          <myip>
            <ip>0.0.0.0</ip>
            <mask>0.0.0.0</mask>
            <gateway>0.0.0.0</gateway>
            <type>ip</type>
          </myip>
          <VLAN
            ID="1">Untagged</VLAN>
        </interface>
      </nic>
      <nic>
        <nictype>port</nictype>
        <nicname>port5</nicname>
        <myid>
          <hostid>118</hostid>
          <nicid>125</nicid>
          <hostname>net_switch1</hostname>
          <nicname>port5</nicname>
        </myid>
        <nictype>port</nictype>
        <uniqueidentifier>125</uniqueidentifier>
        <usesdhcp>False</usesdhcp>
        <encryptionkey />
        <interface>
          <nicname>port5</nicname>
          <myip>
            <ip>0.0.0.0</ip>
            <mask>0.0.0.0</mask>
            <gateway>0.0.0.0</gateway>
            <type>ip</type>
          </myip>
          <VLAN
            ID="1">Untagged</VLAN>
        </interface>
      </nic>
      <nic>
        <nictype>port</nictype>
        <nicname>port6</nicname>
        <myid>
          <hostid>118</hostid>
          <nicid>126</nicid>
          <hostname>net_switch1</hostname>
          <nicname>port6</nicname>
        </myid>
        <nictype>port</nictype>
        <uniqueidentifier>126</uniqueidentifier>
        <usesdhcp>False</usesdhcp>
        <encryptionkey />
        <interface>
          <nicname>port6</nicname>
          <myip>
            <ip>0.0.0.0</ip>
            <mask>0.0.0.0</mask>
            <gateway>0.0.0.0</gateway>
            <type>ip</type>
          </myip>
          <VLAN
            ID="1">Untagged</VLAN>
        </interface>
      </nic>
      <nic>
        <nictype>port</nictype>
        <nicname>port7</nicname>
        <myid>
          <hostid>118</hostid>
          <nicid>127</nicid>
          <hostname>net_switch1</hostname>
          <nicname>port7</nicname>
        </myid>
        <nictype>port</nictype>
        <uniqueidentifier>127</uniqueidentifier>
        <usesdhcp>False</usesdhcp>
        <encryptionkey />
        <interface>
          <nicname>port7</nicname>
          <myip>
            <ip>0.0.0.0</ip>
            <mask>0.0.0.0</mask>
            <gateway>0.0.0.0</gateway>
            <type>ip</type>
          </myip>
          <VLAN
            ID="1">Untagged</VLAN>
        </interface>
      </nic>
    </device>
    <device>
      <hostname>net_switch2</hostname>
      <size>100</size>
      <uniqueidentifier>139</uniqueidentifier>
      <location>640,410</location>
      <mytype>net_switch</mytype>
      <isdns>False</isdns>
      <isdhcp>False</isdhcp>
      <gateway>
        <ip>0.0.0.0</ip>
        <mask>0.0.0.0</mask>
        <gateway>0.0.0.0</gateway>
        <type>gw</type>
      </gateway>
      <nic>
        <nictype>lo</nictype>
        <nicname>lo0</nicname>
        <myid>
          <hostid>139</hostid>
          <nicid>140</nicid>
          <hostname>net_switch2</hostname>
          <nicname>lo0</nicname>
        </myid>
        <nictype>lo</nictype>
        <uniqueidentifier>140</uniqueidentifier>
        <usesdhcp>False</usesdhcp>
        <encryptionkey />
        <interface>
          <nicname>lo0</nicname>
          <myip>
            <ip>127.0.0.1</ip>
            <mask>255.0.0.0</mask>
            <gateway>0.0.0.0</gateway>
            <type>ip</type>
          </myip>
          <VLAN
            ID="1">Untagged</VLAN>
        </interface>
      </nic>
      <nic>
        <nictype>management_interface</nictype>
        <nicname>management_interface0</nicname>
        <myid>
          <hostid>139</hostid>
          <nicid>141</nicid>
          <hostname>net_switch2</hostname>
          <nicname>management_interface0</nicname>
        </myid>
        <nictype>management_interface</nictype>
        <uniqueidentifier>141</uniqueidentifier>
        <usesdhcp>False</usesdhcp>
        <encryptionkey />
        <interface>
          <nicname>management_interface0</nicname>
          <myip>
            <ip>0.0.0.0</ip>
            <mask>0.0.0.0</mask>
            <gateway>0.0.0.0</gateway>
            <type>ip</type>
          </myip>
          <VLAN
            ID="1">Untagged</VLAN>
        </interface>
      </nic>
      <nic>
        <nictype>port</nictype>
        <nicname>port1</nicname>
        <myid>
          <hostid>139</hostid>
          <nicid>142</nicid>
          <hostname>net_switch2</hostname>
          <nicname>port1</nicname>
        </myid>
        <nictype>port</nictype>
        <uniqueidentifier>142</uniqueidentifier>
        <usesdhcp>False</usesdhcp>
        <encryptionkey />
        <interface>
          <nicname>port1</nicname>
          <myip>
            <ip>0.0.0.0</ip>
            <mask>0.0.0.0</mask>
            <gateway>0.0.0.0</gateway>
            <type>ip</type>
          </myip>
          <VLAN
            ID="1">Untagged</VLAN>
        </interface>
      </nic>
      <nic>
        <nictype>port</nictype>
        <nicname>port2</nicname>
        <myid>
          <hostid>139</hostid>
          <nicid>143</nicid>
          <hostname>net_switch2</hostname>
          <nicname>port2</nicname>
        </myid>
        <nictype>port</nictype>
        <uniqueidentifier>143</uniqueidentifier>
        <usesdhcp>False</usesdhcp>
        <encryptionkey />
        <interface>
          <nicname>port2</nicname>
          <myip>
            <ip>0.0.0.0</ip>
            <mask>0.0.0.0</mask>
            <gateway>0.0.0.0</gateway>
            <type>ip</type>
          </myip>
          <VLAN
            ID="1">Untagged</VLAN>
        </interface>
      </nic>
      <nic>
        <nictype>port</nictype>
        <nicname>port3</nicname>
        <myid>
          <hostid>139</hostid>
          <nicid>144</nicid>
          <hostname>net_switch2</hostname>
          <nicname>port3</nicname>
        </myid>
        <nictype>port</nictype>
        <uniqueidentifier>144</uniqueidentifier>
        <usesdhcp>False</usesdhcp>
        <encryptionkey />
        <interface>
          <nicname>port3</nicname>
          <myip>
            <ip>0.0.0.0</ip>
            <mask>0.0.0.0</mask>
            <gateway>0.0.0.0</gateway>
            <type>ip</type>
          </myip>
          <VLAN
            ID="1">Untagged</VLAN>
        </interface>
      </nic>
      <nic>
        <nictype>port</nictype>
        <nicname>port4</nicname>
        <myid>
          <hostid>139</hostid>
          <nicid>145</nicid>
          <hostname>net_switch2</hostname>
          <nicname>port4</nicname>
        </myid>
        <nictype>port</nictype>
        <uniqueidentifier>145</uniqueidentifier>
        <usesdhcp>False</usesdhcp>
        <encryptionkey />
        <interface>
          <nicname>port4</nicname>
          <myip>
            <ip>0.0.0.0</ip>
            <mask>0.0.0.0</mask>
            <gateway>0.0.0.0</gateway>
            <type>ip</type>
          </myip>
          <VLAN
            ID="1">Untagged</VLAN>
        </interface>
      </nic>
      <nic>
        <nictype>port</nictype>
        <nicname>port5</nicname>
        <myid>
          <hostid>139</hostid>
          <nicid>146</nicid>
          <hostname>net_switch2</hostname>
          <nicname>port5</nicname>
        </myid>
        <nictype>port</nictype>
        <uniqueidentifier>146</uniqueidentifier>
        <usesdhcp>False</usesdhcp>
        <encryptionkey />
        <interface>
          <nicname>port5</nicname>
          <myip>
            <ip>0.0.0.0</ip>
            <mask>0.0.0.0</mask>
            <gateway>0.0.0.0</gateway>
            <type>ip</type>
          </myip>
          <VLAN
            ID="1">Untagged</VLAN>
        </interface>
      </nic>
      <nic>
        <nictype>port</nictype>
        <nicname>port6</nicname>
        <myid>
          <hostid>139</hostid>
          <nicid>147</nicid>
          <hostname>net_switch2</hostname>
          <nicname>port6</nicname>
        </myid>
        <nictype>port</nictype>
        <uniqueidentifier>147</uniqueidentifier>
        <usesdhcp>False</usesdhcp>
        <encryptionkey />
        <interface>
          <nicname>port6</nicname>
          <myip>
            <ip>0.0.0.0</ip>
            <mask>0.0.0.0</mask>
            <gateway>0.0.0.0</gateway>
            <type>ip</type>
          </myip>
          <VLAN
            ID="1">Untagged</VLAN>
        </interface>
      </nic>
      <nic>
        <nictype>port</nictype>
        <nicname>port7</nicname>
        <myid>
          <hostid>139</hostid>
          <nicid>148</nicid>
          <hostname>net_switch2</hostname>
          <nicname>port7</nicname>
        </myid>
        <nictype>port</nictype>
        <uniqueidentifier>148</uniqueidentifier>
        <usesdhcp>False</usesdhcp>
        <encryptionkey />
        <interface>
          <nicname>port7</nicname>
          <myip>
            <ip>0.0.0.0</ip>
            <mask>0.0.0.0</mask>
            <gateway>0.0.0.0</gateway>
            <type>ip</type>
          </myip>
          <VLAN
            ID="1">Untagged</VLAN>
        </interface>
      </nic>
    </device>
    <device>
      <hostname>pc0</hostname>
      <size>100</size>
      <uniqueidentifier>115</uniqueidentifier>
      <location>640,190</location>
      <mytype>pc</mytype>
      <isdns>False</isdns>
      <isdhcp>False</isdhcp>
      <gateway>
        <ip>192.168.5.1</ip>
        <mask>0.0.0.0</mask>
        <gateway>0.0.0.0</gateway>
        <type>gw</type>
      </gateway>
      <nic>
        <nictype>lo</nictype>
        <nicname>lo0</nicname>
        <myid>
          <hostid>115</hostid>
          <nicid>116</nicid>
          <hostname>pc0</hostname>
          <nicname>lo0</nicname>
        </myid>
        <nictype>lo</nictype>
        <uniqueidentifier>116</uniqueidentifier>
        <usesdhcp>False</usesdhcp>
        <encryptionkey />
        <interface>
          <nicname>lo0</nicname>
          <myip>
            <ip>127.0.0.1</ip>
            <mask>255.0.0.0</mask>
            <gateway>0.0.0.0</gateway>
            <type>ip</type>
          </myip>
          <VLAN
            ID="1">Untagged</VLAN>
        </interface>
      </nic>
      <nic>
        <nictype>eth</nictype>
        <nicname>eth0</nicname>
        <myid>
          <hostid>115</hostid>
          <nicid>117</nicid>
          <hostname>pc0</hostname>
          <nicname>eth0</nicname>
        </myid>
        <nictype>eth</nictype>
        <uniqueidentifier>117</uniqueidentifier>
        <usesdhcp>False</usesdhcp>
        <encryptionkey />
        <interface>
          <nicname>eth0</nicname>
          <myip>
            <ip>192.168.5.2</ip>
            <mask>255.255.255.0</mask>
            <gateway>0.0.0.0</gateway>
            <type>ip</type>
          </myip>
          <VLAN
            ID="1">Untagged</VLAN>
        </interface>
      </nic>
    </device>
    <device>
      <hostname>pc1</hostname>
      <size>100</size>
      <uniqueidentifier>128</uniqueidentifier>
      <location>230,600</location>
      <mytype>pc</mytype>
      <isdns>False</isdns>
      <isdhcp>False</isdhcp>
      <gateway>
        <ip>192.168.1.1</ip>
        <mask>0.0.0.0</mask>
        <gateway>0.0.0.0</gateway>
        <type>gw</type>
      </gateway>
      <nic>
        <nictype>lo</nictype>
        <nicname>lo0</nicname>
        <myid>
          <hostid>128</hostid>
          <nicid>129</nicid>
          <hostname>pc1</hostname>
          <nicname>lo0</nicname>
        </myid>
        <nictype>lo</nictype>
        <uniqueidentifier>129</uniqueidentifier>
        <usesdhcp>False</usesdhcp>
        <encryptionkey />
        <interface>
          <nicname>lo0</nicname>
          <myip>
            <ip>127.0.0.1</ip>
            <mask>255.0.0.0</mask>
            <gateway>0.0.0.0</gateway>
            <type>ip</type>
          </myip>
          <VLAN
            ID="1">Untagged</VLAN>
        </interface>
      </nic>
      <nic>
        <nictype>eth</nictype>
        <nicname>eth0</nicname>
        <myid>
          <hostid>128</hostid>
          <nicid>130</nicid>
          <hostname>pc1</hostname>
          <nicname>eth0</nicname>
        </myid>
        <nictype>eth</nictype>
        <uniqueidentifier>130</uniqueidentifier>
        <usesdhcp>False</usesdhcp>
        <encryptionkey />
        <interface>
          <nicname>eth0</nicname>
          <myip>
            <ip>192.168.1.2</ip>
            <mask>255.255.255.0</mask>
            <gateway>0.0.0.0</gateway>
            <type>ip</type>
          </myip>
          <VLAN
            ID="1">Untagged</VLAN>
        </interface>
      </nic>
    </device>
    <device>
      <hostname>pc2</hostname>
      <size>100</size>
      <uniqueidentifier>135</uniqueidentifier>
      <location>90,590</location>
      <mytype>pc</mytype>
      <isdns>False</isdns>
      <isdhcp>False</isdhcp>
      <gateway>
        <ip>0.0.0.0</ip>
        <mask>0.0.0.0</mask>
        <gateway>0.0.0.0</gateway>
        <type>gw</type>
      </gateway>
      <nic>
        <nictype>lo</nictype>
        <nicname>lo0</nicname>
        <myid>
          <hostid>135</hostid>
          <nicid>136</nicid>
          <hostname>pc2</hostname>
          <nicname>lo0</nicname>
        </myid>
        <nictype>lo</nictype>
        <uniqueidentifier>136</uniqueidentifier>
        <usesdhcp>False</usesdhcp>
        <encryptionkey />
        <interface>
          <nicname>lo0</nicname>
          <myip>
            <ip>127.0.0.1</ip>
            <mask>255.0.0.0</mask>
            <gateway>0.0.0.0</gateway>
            <type>ip</type>
          </myip>
          <VLAN
            ID="1">Untagged</VLAN>
        </interface>
      </nic>
      <nic>
        <nictype>eth</nictype>
        <nicname>eth0</nicname>
        <myid>
          <hostid>135</hostid>
          <nicid>137</nicid>
          <hostname>pc2</hostname>
          <nicname>eth0</nicname>
        </myid>
        <nictype>eth</nictype>
        <uniqueidentifier>137</uniqueidentifier>
        <usesdhcp>True</usesdhcp>
        <encryptionkey />
        <interface>
          <nicname>eth0</nicname>
          <myip>
            <ip>0.0.0.0</ip>
            <mask>0.0.0.0</mask>
            <gateway>0.0.0.0</gateway>
            <type>ip</type>
          </myip>
          <VLAN
            ID="1">Untagged</VLAN>
        </interface>
      </nic>
    </device>
    <device>
      <hostname>pc3</hostname>
      <size>100</size>
      <uniqueidentifier>149</uniqueidentifier>
      <location>640,600</location>
      <mytype>pc</mytype>
      <isdns>False</isdns>
      <isdhcp>False</isdhcp>
      <gateway>
        <ip>192.168.2.1</ip>
        <mask>0.0.0.0</mask>
        <gateway>0.0.0.0</gateway>
        <type>gw</type>
      </gateway>
      <nic>
        <nictype>lo</nictype>
        <nicname>lo0</nicname>
        <myid>
          <hostid>149</hostid>
          <nicid>150</nicid>
          <hostname>pc3</hostname>
          <nicname>lo0</nicname>
        </myid>
        <nictype>lo</nictype>
        <uniqueidentifier>150</uniqueidentifier>
        <usesdhcp>False</usesdhcp>
        <encryptionkey />
        <interface>
          <nicname>lo0</nicname>
          <myip>
            <ip>127.0.0.1</ip>
            <mask>255.0.0.0</mask>
            <gateway>0.0.0.0</gateway>
            <type>ip</type>
          </myip>
          <VLAN
            ID="1">Untagged</VLAN>
        </interface>
      </nic>
      <nic>
        <nictype>eth</nictype>
        <nicname>eth0</nicname>
        <myid>
          <hostid>149</hostid>
          <nicid>151</nicid>
          <hostname>pc3</hostname>
          <nicname>eth0</nicname>
        </myid>
        <nictype>eth</nictype>
        <uniqueidentifier>151</uniqueidentifier>
        <usesdhcp>False</usesdhcp>
        <encryptionkey />
        <interface>
          <nicname>eth0</nicname>
          <myip>
            <ip>192.168.2.2</ip>
            <mask>255.255.255.0</mask>
            <gateway>0.0.0.0</gateway>
            <type>ip</type>
          </myip>
          <VLAN
            ID="1">Untagged</VLAN>
        </interface>
      </nic>
    </device>
    <device>
      <hostname>pc4</hostname>
      <size>100</size>
      <uniqueidentifier>154</uniqueidentifier>
      <location>760,600</location>
      <mytype>pc</mytype>
      <isdns>False</isdns>
      <isdhcp>False</isdhcp>
      <gateway>
        <ip>0.0.0.0</ip>
        <mask>0.0.0.0</mask>
        <gateway>0.0.0.0</gateway>
        <type>gw</type>
      </gateway>
      <nic>
        <nictype>lo</nictype>
        <nicname>lo0</nicname>
        <myid>
          <hostid>154</hostid>
          <nicid>155</nicid>
          <hostname>pc4</hostname>
          <nicname>lo0</nicname>
        </myid>
        <nictype>lo</nictype>
        <uniqueidentifier>155</uniqueidentifier>
        <usesdhcp>False</usesdhcp>
        <encryptionkey />
        <interface>
          <nicname>lo0</nicname>
          <myip>
            <ip>127.0.0.1</ip>
            <mask>255.0.0.0</mask>
            <gateway>0.0.0.0</gateway>
            <type>ip</type>
          </myip>
          <VLAN
            ID="1">Untagged</VLAN>
        </interface>
      </nic>
      <nic>
        <nictype>eth</nictype>
        <nicname>eth0</nicname>
        <myid>
          <hostid>154</hostid>
          <nicid>156</nicid>
          <hostname>pc4</hostname>
          <nicname>eth0</nicname>
        </myid>
        <nictype>eth</nictype>
        <uniqueidentifier>156</uniqueidentifier>
        <usesdhcp>True</usesdhcp>
        <encryptionkey />
        <interface>
          <nicname>eth0</nicname>
          <myip>
            <ip>0.0.0.0</ip>
            <mask>0.0.0.0</mask>
            <gateway>0.0.0.0</gateway>
            <type>ip</type>
          </myip>
          <VLAN
            ID="1">Untagged</VLAN>
        </interface>
      </nic>
    </device>
    <link>
      <SrcNic>
        <hostid>128</hostid>
        <nicid>130</nicid>
        <hostname>pc1</hostname>
        <nicname>eth0</nicname>
      </SrcNic>
      <DstNic>
        <hostid>118</hostid>
        <nicid>121</nicid>
        <hostname>net_switch1</hostname>
        <nicname>port1</nicname>
      </DstNic>
      <hostname>pc1_link_net_switch1</hostname>
      <linktype>normal</linktype>
      <uniqueidentifier>131</uniqueidentifier>
    </link>
    <link>
      <SrcNic>
        <hostid>118</hostid>
        <nicid>122</nicid>
        <hostname>net_switch1</hostname>
        <nicname>port2</nicname>
      </SrcNic>
      <DstNic>
        <hostid>100</hostid>
        <nicid>102</nicid>
        <hostname>firewall0</hostname>
        <nicname>eth0</nicname>
      </DstNic>
      <hostname>net_switch1_link_firewall0</hostname>
      <linktype>normal</linktype>
      <uniqueidentifier>132</uniqueidentifier>
    </link>
    <link>
      <SrcNic>
        <hostid>100</hostid>
        <nicid>104</nicid>
        <hostname>firewall0</hostname>
        <nicname>wan0</nicname>
      </SrcNic>
      <DstNic>
        <hostid>105</hostid>
        <nicid>108</nicid>
        <hostname>net_switch0</hostname>
        <nicname>port1</nicname>
      </DstNic>
      <hostname>firewall0_link_net_switch0</hostname>
      <linktype>normal</linktype>
      <uniqueidentifier>133</uniqueidentifier>
    </link>
    <link>
      <SrcNic>
        <hostid>105</hostid>
        <nicid>109</nicid>
        <hostname>net_switch0</hostname>
        <nicname>port2</nicname>
      </SrcNic>
      <DstNic>
        <hostid>115</hostid>
        <nicid>117</nicid>
        <hostname>pc0</hostname>
        <nicname>eth0</nicname>
      </DstNic>
      <hostname>net_switch0_link_pc0</hostname>
      <linktype>normal</linktype>
      <uniqueidentifier>134</uniqueidentifier>
    </link>
    <link>
      <SrcNic>
        <hostid>135</hostid>
        <nicid>137</nicid>
        <hostname>pc2</hostname>
        <nicname>eth0</nicname>
      </SrcNic>
      <DstNic>
        <hostid>118</hostid>
        <nicid>123</nicid>
        <hostname>net_switch1</hostname>
        <nicname>port3</nicname>
      </DstNic>
      <hostname>pc2_link_net_switch1</hostname>
      <linktype>normal</linktype>
      <uniqueidentifier>138</uniqueidentifier>
    </link>
    <link>
      <SrcNic>
        <hostid>100</hostid>
        <nicid>103</nicid>
        <hostname>firewall0</hostname>
        <nicname>eth1</nicname>
      </SrcNic>
      <DstNic>
        <hostid>139</hostid>
        <nicid>142</nicid>
        <hostname>net_switch2</hostname>
        <nicname>port1</nicname>
      </DstNic>
      <hostname>firewall0_link_net_switch2</hostname>
      <linktype>normal</linktype>
      <uniqueidentifier>152</uniqueidentifier>
    </link>
    <link>
      <SrcNic>
        <hostid>139</hostid>
        <nicid>143</nicid>
        <hostname>net_switch2</hostname>
        <nicname>port2</nicname>
      </SrcNic>
      <DstNic>
        <hostid>149</hostid>
        <nicid>151</nicid>
        <hostname>pc3</hostname>
        <nicname>eth0</nicname>
      </DstNic>
      <hostname>net_switch2_link_pc3</hostname>
      <linktype>normal</linktype>
      <uniqueidentifier>153</uniqueidentifier>
    </link>
    <link>
      <SrcNic>
        <hostid>154</hostid>
        <nicid>156</nicid>
        <hostname>pc4</hostname>
        <nicname>eth0</nicname>
      </SrcNic>
      <DstNic>
        <hostid>139</hostid>
        <nicid>144</nicid>
        <hostname>net_switch2</hostname>
        <nicname>port3</nicname>
      </DstNic>
      <hostname>pc4_link_net_switch2</hostname>
      <linktype>normal</linktype>
      <uniqueidentifier>157</uniqueidentifier>
    </link>
    <nettest>
      <shost>pc1</shost>
      <dhost>pc3</dhost>
      <thetest>SuccessfullyPings</thetest>
    </nettest>
    <nettest>
      <shost>pc3</shost>
      <dhost>pc1</dhost>
      <thetest>SuccessfullyPings</thetest>
    </nettest>
    <tag>Firewall</tag>
    <tag>Ping</tag>
    <VLANName
      ID="1"
      Color="Blue">Default</VLANName>
  </Network>
</EduNetworkBuilder>