<?xml version="1.0" encoding="utf-8"?>
<EduNetworkBuilder>
  <!--This is a network file for EduNetworkBuilder.-->
  <Network>
    <fr_message>Le sans fil peut être affecté par d'autres choses qui produisent des interférences. Déterminez l'origine du problème et résolvez le problème.</fr_message>
    <en_message>Wireless can be affected by other things that produce interference.  Determine what is causing the problem and fix the problem.</en_message>
    <en_title>Wireless Corruption</en_title>
    <en_url />
    <height>1024</height>
    <width>1024</width>
    <itemsize>100</itemsize>
    <showlabels>full</showlabels>
    <level>5</level>
    <sortorder>7</sortorder>
    <uniqueidentifier>340</uniqueidentifier>
    <startinghelplevel>full</startinghelplevel>
    <vlansenabled>True</vlansenabled>
    <VLANPacketColors>False</VLANPacketColors>
    <device>
      <hostname>laptop1</hostname>
      <size>100</size>
      <uniqueidentifier>143</uniqueidentifier>
      <location>800,850</location>
      <mytype>laptop</mytype>
      <isdns>False</isdns>
      <isdhcp>False</isdhcp>
      <gateway>
        <ip>192.168.2.1</ip>
        <mask>0.0.0.0</mask>
        <gateway>0.0.0.0</gateway>
        <type>gw</type>
      </gateway>
      <nic>
        <nictype>lo</nictype>
        <nicname>lo0</nicname>
        <myid>
          <hostid>143</hostid>
          <nicid>144</nicid>
          <hostname>laptop1</hostname>
          <nicname>lo0</nicname>
        </myid>
        <nictype>lo</nictype>
        <uniqueidentifier>144</uniqueidentifier>
        <usesdhcp>False</usesdhcp>
        <encryptionkey />
        <ssid />
        <interface>
          <nicname>lo0</nicname>
          <myip>
            <ip>127.0.0.1</ip>
            <mask>255.0.0.0</mask>
            <gateway>0.0.0.0</gateway>
            <type>ip</type>
          </myip>
          <VLAN
            ID="1">Untagged</VLAN>
        </interface>
      </nic>
      <nic>
        <nictype>eth</nictype>
        <nicname>eth0</nicname>
        <myid>
          <hostid>143</hostid>
          <nicid>145</nicid>
          <hostname>laptop1</hostname>
          <nicname>eth0</nicname>
        </myid>
        <nictype>eth</nictype>
        <uniqueidentifier>145</uniqueidentifier>
        <usesdhcp>False</usesdhcp>
        <encryptionkey />
        <ssid />
        <interface>
          <nicname>eth0</nicname>
          <myip>
            <ip>192.168.2.3</ip>
            <mask>255.255.255.0</mask>
            <gateway>0.0.0.0</gateway>
            <type>ip</type>
          </myip>
          <VLAN
            ID="1">Untagged</VLAN>
        </interface>
      </nic>
    </device>
    <device>
      <hostname>net_switch1</hostname>
      <size>100</size>
      <uniqueidentifier>124</uniqueidentifier>
      <location>700,690</location>
      <mytype>net_switch</mytype>
      <isdns>False</isdns>
      <isdhcp>False</isdhcp>
      <gateway>
        <ip>192.168.2.1</ip>
        <mask>0.0.0.0</mask>
        <gateway>0.0.0.0</gateway>
        <type>gw</type>
      </gateway>
      <nic>
        <nictype>lo</nictype>
        <nicname>lo0</nicname>
        <myid>
          <hostid>124</hostid>
          <nicid>125</nicid>
          <hostname>net_switch1</hostname>
          <nicname>lo0</nicname>
        </myid>
        <nictype>lo</nictype>
        <uniqueidentifier>125</uniqueidentifier>
        <usesdhcp>False</usesdhcp>
        <encryptionkey />
        <ssid />
        <interface>
          <nicname>lo0</nicname>
          <myip>
            <ip>127.0.0.1</ip>
            <mask>255.0.0.0</mask>
            <gateway>0.0.0.0</gateway>
            <type>ip</type>
          </myip>
          <VLAN
            ID="1">Untagged</VLAN>
        </interface>
      </nic>
      <nic>
        <nictype>management_interface</nictype>
        <nicname>management_interface0</nicname>
        <myid>
          <hostid>124</hostid>
          <nicid>126</nicid>
          <hostname>net_switch1</hostname>
          <nicname>management_interface0</nicname>
        </myid>
        <nictype>management_interface</nictype>
        <uniqueidentifier>126</uniqueidentifier>
        <usesdhcp>False</usesdhcp>
        <encryptionkey />
        <ssid />
        <interface>
          <nicname>management_interface0</nicname>
          <myip>
            <ip>192.168.2.4</ip>
            <mask>255.255.255.0</mask>
            <gateway>0.0.0.0</gateway>
            <type>ip</type>
          </myip>
          <VLAN
            ID="1">Untagged</VLAN>
        </interface>
      </nic>
      <nic>
        <nictype>port</nictype>
        <nicname>port1</nicname>
        <myid>
          <hostid>124</hostid>
          <nicid>127</nicid>
          <hostname>net_switch1</hostname>
          <nicname>port1</nicname>
        </myid>
        <nictype>port</nictype>
        <uniqueidentifier>127</uniqueidentifier>
        <usesdhcp>False</usesdhcp>
        <encryptionkey />
        <ssid />
        <interface>
          <nicname>port1</nicname>
          <myip>
            <ip>0.0.0.0</ip>
            <mask>0.0.0.0</mask>
            <gateway>0.0.0.0</gateway>
            <type>ip</type>
          </myip>
          <VLAN
            ID="1">Untagged</VLAN>
        </interface>
      </nic>
      <nic>
        <nictype>port</nictype>
        <nicname>port2</nicname>
        <myid>
          <hostid>124</hostid>
          <nicid>128</nicid>
          <hostname>net_switch1</hostname>
          <nicname>port2</nicname>
        </myid>
        <nictype>port</nictype>
        <uniqueidentifier>128</uniqueidentifier>
        <usesdhcp>False</usesdhcp>
        <encryptionkey />
        <ssid />
        <interface>
          <nicname>port2</nicname>
          <myip>
            <ip>0.0.0.0</ip>
            <mask>0.0.0.0</mask>
            <gateway>0.0.0.0</gateway>
            <type>ip</type>
          </myip>
          <VLAN
            ID="1">Untagged</VLAN>
        </interface>
      </nic>
      <nic>
        <nictype>port</nictype>
        <nicname>port3</nicname>
        <myid>
          <hostid>124</hostid>
          <nicid>129</nicid>
          <hostname>net_switch1</hostname>
          <nicname>port3</nicname>
        </myid>
        <nictype>port</nictype>
        <uniqueidentifier>129</uniqueidentifier>
        <usesdhcp>False</usesdhcp>
        <encryptionkey />
        <ssid />
        <interface>
          <nicname>port3</nicname>
          <myip>
            <ip>0.0.0.0</ip>
            <mask>0.0.0.0</mask>
            <gateway>0.0.0.0</gateway>
            <type>ip</type>
          </myip>
          <VLAN
            ID="1">Untagged</VLAN>
        </interface>
      </nic>
      <nic>
        <nictype>port</nictype>
        <nicname>port4</nicname>
        <myid>
          <hostid>124</hostid>
          <nicid>130</nicid>
          <hostname>net_switch1</hostname>
          <nicname>port4</nicname>
        </myid>
        <nictype>port</nictype>
        <uniqueidentifier>130</uniqueidentifier>
        <usesdhcp>False</usesdhcp>
        <encryptionkey />
        <ssid />
        <interface>
          <nicname>port4</nicname>
          <myip>
            <ip>0.0.0.0</ip>
            <mask>0.0.0.0</mask>
            <gateway>0.0.0.0</gateway>
            <type>ip</type>
          </myip>
          <VLAN
            ID="1">Untagged</VLAN>
        </interface>
      </nic>
      <nic>
        <nictype>port</nictype>
        <nicname>port5</nicname>
        <myid>
          <hostid>124</hostid>
          <nicid>131</nicid>
          <hostname>net_switch1</hostname>
          <nicname>port5</nicname>
        </myid>
        <nictype>port</nictype>
        <uniqueidentifier>131</uniqueidentifier>
        <usesdhcp>False</usesdhcp>
        <encryptionkey />
        <ssid />
        <interface>
          <nicname>port5</nicname>
          <myip>
            <ip>0.0.0.0</ip>
            <mask>0.0.0.0</mask>
            <gateway>0.0.0.0</gateway>
            <type>ip</type>
          </myip>
          <VLAN
            ID="1">Untagged</VLAN>
        </interface>
      </nic>
      <nic>
        <nictype>port</nictype>
        <nicname>port6</nicname>
        <myid>
          <hostid>124</hostid>
          <nicid>132</nicid>
          <hostname>net_switch1</hostname>
          <nicname>port6</nicname>
        </myid>
        <nictype>port</nictype>
        <uniqueidentifier>132</uniqueidentifier>
        <usesdhcp>False</usesdhcp>
        <encryptionkey />
        <ssid />
        <interface>
          <nicname>port6</nicname>
          <myip>
            <ip>0.0.0.0</ip>
            <mask>0.0.0.0</mask>
            <gateway>0.0.0.0</gateway>
            <type>ip</type>
          </myip>
          <VLAN
            ID="1">Untagged</VLAN>
        </interface>
      </nic>
      <nic>
        <nictype>port</nictype>
        <nicname>port7</nicname>
        <myid>
          <hostid>124</hostid>
          <nicid>133</nicid>
          <hostname>net_switch1</hostname>
          <nicname>port7</nicname>
        </myid>
        <nictype>port</nictype>
        <uniqueidentifier>133</uniqueidentifier>
        <usesdhcp>False</usesdhcp>
        <encryptionkey />
        <ssid />
        <interface>
          <nicname>port7</nicname>
          <myip>
            <ip>0.0.0.0</ip>
            <mask>0.0.0.0</mask>
            <gateway>0.0.0.0</gateway>
            <type>ip</type>
          </myip>
          <VLAN
            ID="1">Untagged</VLAN>
        </interface>
      </nic>
    </device>
    <device>
      <hostname>pc1</hostname>
      <size>100</size>
      <uniqueidentifier>137</uniqueidentifier>
      <location>600,850</location>
      <mytype>pc</mytype>
      <isdns>False</isdns>
      <isdhcp>False</isdhcp>
      <gateway>
        <ip>192.168.2.1</ip>
        <mask>0.0.0.0</mask>
        <gateway>0.0.0.0</gateway>
        <type>gw</type>
      </gateway>
      <nic>
        <nictype>lo</nictype>
        <nicname>lo0</nicname>
        <myid>
          <hostid>137</hostid>
          <nicid>138</nicid>
          <hostname>pc1</hostname>
          <nicname>lo0</nicname>
        </myid>
        <nictype>lo</nictype>
        <uniqueidentifier>138</uniqueidentifier>
        <usesdhcp>False</usesdhcp>
        <encryptionkey />
        <ssid />
        <interface>
          <nicname>lo0</nicname>
          <myip>
            <ip>127.0.0.1</ip>
            <mask>255.0.0.0</mask>
            <gateway>0.0.0.0</gateway>
            <type>ip</type>
          </myip>
          <VLAN
            ID="1">Untagged</VLAN>
        </interface>
      </nic>
      <nic>
        <nictype>eth</nictype>
        <nicname>eth0</nicname>
        <myid>
          <hostid>137</hostid>
          <nicid>139</nicid>
          <hostname>pc1</hostname>
          <nicname>eth0</nicname>
        </myid>
        <nictype>eth</nictype>
        <uniqueidentifier>139</uniqueidentifier>
        <usesdhcp>False</usesdhcp>
        <encryptionkey />
        <ssid />
        <interface>
          <nicname>eth0</nicname>
          <myip>
            <ip>192.168.2.2</ip>
            <mask>255.255.255.0</mask>
            <gateway>0.0.0.0</gateway>
            <type>ip</type>
          </myip>
          <VLAN
            ID="1">Untagged</VLAN>
        </interface>
      </nic>
    </device>
    <device>
      <hostname>pc3</hostname>
      <size>100</size>
      <uniqueidentifier>243</uniqueidentifier>
      <location>400,180</location>
      <mytype>pc</mytype>
      <isdns>False</isdns>
      <isdhcp>False</isdhcp>
      <gateway>
        <ip>192.168.2.1</ip>
        <mask>0.0.0.0</mask>
        <gateway>0.0.0.0</gateway>
        <type>gw</type>
      </gateway>
      <nic>
        <nictype>lo</nictype>
        <nicname>lo0</nicname>
        <myid>
          <hostid>243</hostid>
          <nicid>244</nicid>
          <hostname>pc3</hostname>
          <nicname>lo0</nicname>
        </myid>
        <nictype>lo</nictype>
        <uniqueidentifier>244</uniqueidentifier>
        <usesdhcp>False</usesdhcp>
        <interface>
          <nicname>lo0</nicname>
          <myip>
            <ip>127.0.0.1</ip>
            <mask>255.0.0.0</mask>
            <gateway>0.0.0.0</gateway>
            <type>ip</type>
          </myip>
          <VLAN
            ID="1">Untagged</VLAN>
        </interface>
      </nic>
      <nic>
        <nictype>eth</nictype>
        <nicname>eth0</nicname>
        <myid>
          <hostid>243</hostid>
          <nicid>245</nicid>
          <hostname>pc3</hostname>
          <nicname>eth0</nicname>
        </myid>
        <nictype>eth</nictype>
        <uniqueidentifier>245</uniqueidentifier>
        <usesdhcp>False</usesdhcp>
        <interface>
          <nicname>eth0</nicname>
          <myip>
            <ip>192.168.2.6</ip>
            <mask>255.255.255.0</mask>
            <gateway>0.0.0.0</gateway>
            <type>ip</type>
          </myip>
          <VLAN
            ID="1">Untagged</VLAN>
        </interface>
      </nic>
    </device>
    <device>
      <hostname>printer0</hostname>
      <size>100</size>
      <uniqueidentifier>256</uniqueidentifier>
      <location>390,20</location>
      <mytype>printer</mytype>
      <isdns>False</isdns>
      <isdhcp>False</isdhcp>
      <gateway>
        <ip>192.168.2.1</ip>
        <mask>0.0.0.0</mask>
        <gateway>0.0.0.0</gateway>
        <type>gw</type>
      </gateway>
      <nic>
        <nictype>lo</nictype>
        <nicname>lo0</nicname>
        <myid>
          <hostid>256</hostid>
          <nicid>257</nicid>
          <hostname>printer0</hostname>
          <nicname>lo0</nicname>
        </myid>
        <nictype>lo</nictype>
        <uniqueidentifier>257</uniqueidentifier>
        <usesdhcp>False</usesdhcp>
        <interface>
          <nicname>lo0</nicname>
          <myip>
            <ip>127.0.0.1</ip>
            <mask>255.0.0.0</mask>
            <gateway>0.0.0.0</gateway>
            <type>ip</type>
          </myip>
          <VLAN
            ID="1">Untagged</VLAN>
        </interface>
      </nic>
      <nic>
        <nictype>eth</nictype>
        <nicname>eth0</nicname>
        <myid>
          <hostid>256</hostid>
          <nicid>258</nicid>
          <hostname>printer0</hostname>
          <nicname>eth0</nicname>
        </myid>
        <nictype>eth</nictype>
        <uniqueidentifier>258</uniqueidentifier>
        <usesdhcp>False</usesdhcp>
        <interface>
          <nicname>eth0</nicname>
          <myip>
            <ip>192.168.2.7</ip>
            <mask>255.255.255.0</mask>
            <gateway>0.0.0.0</gateway>
            <type>ip</type>
          </myip>
          <VLAN
            ID="1">Untagged</VLAN>
        </interface>
      </nic>
    </device>
    <device>
      <hostname>wbridge0</hostname>
      <size>100</size>
      <uniqueidentifier>232</uniqueidentifier>
      <location>120,80</location>
      <mytype>wbridge</mytype>
      <isdns>False</isdns>
      <isdhcp>False</isdhcp>
      <gateway>
        <ip>192.168.2.1</ip>
        <mask>0.0.0.0</mask>
        <gateway>0.0.0.0</gateway>
        <type>gw</type>
      </gateway>
      <nic>
        <nictype>lo</nictype>
        <nicname>lo0</nicname>
        <myid>
          <hostid>232</hostid>
          <nicid>235</nicid>
          <hostname>wbridge0</hostname>
          <nicname>lo0</nicname>
        </myid>
        <nictype>lo</nictype>
        <uniqueidentifier>235</uniqueidentifier>
        <usesdhcp>False</usesdhcp>
        <interface>
          <nicname>lo0</nicname>
          <myip>
            <ip>127.0.0.1</ip>
            <mask>255.0.0.0</mask>
            <gateway>0.0.0.0</gateway>
            <type>ip</type>
          </myip>
          <VLAN
            ID="1">Untagged</VLAN>
        </interface>
      </nic>
      <nic>
        <nictype>wlan</nictype>
        <nicname>wlan1</nicname>
        <myid>
          <hostid>232</hostid>
          <nicid>236</nicid>
          <hostname>wbridge0</hostname>
          <nicname>wlan1</nicname>
        </myid>
        <nictype>wlan</nictype>
        <uniqueidentifier>236</uniqueidentifier>
        <usesdhcp>False</usesdhcp>
        <encryptionkey>myKey</encryptionkey>
        <ssid>my_SSID</ssid>
        <interface>
          <nicname>wlan1</nicname>
          <myip>
            <ip>192.168.2.5</ip>
            <mask>255.255.255.0</mask>
            <gateway>0.0.0.0</gateway>
            <type>ip</type>
          </myip>
          <VLAN
            ID="1">Untagged</VLAN>
        </interface>
      </nic>
      <nic>
        <nictype>port</nictype>
        <nicname>port2</nicname>
        <myid>
          <hostid>232</hostid>
          <nicid>237</nicid>
          <hostname>wbridge0</hostname>
          <nicname>port2</nicname>
        </myid>
        <nictype>port</nictype>
        <uniqueidentifier>237</uniqueidentifier>
        <usesdhcp>False</usesdhcp>
        <interface>
          <nicname>port2</nicname>
          <myip>
            <ip>0.0.0.0</ip>
            <mask>0.0.0.0</mask>
            <gateway>0.0.0.0</gateway>
            <type>ip</type>
          </myip>
          <VLAN
            ID="1">Untagged</VLAN>
        </interface>
      </nic>
      <nic>
        <nictype>port</nictype>
        <nicname>port3</nicname>
        <myid>
          <hostid>232</hostid>
          <nicid>238</nicid>
          <hostname>wbridge0</hostname>
          <nicname>port3</nicname>
        </myid>
        <nictype>port</nictype>
        <uniqueidentifier>238</uniqueidentifier>
        <usesdhcp>False</usesdhcp>
        <interface>
          <nicname>port3</nicname>
          <myip>
            <ip>0.0.0.0</ip>
            <mask>0.0.0.0</mask>
            <gateway>0.0.0.0</gateway>
            <type>ip</type>
          </myip>
          <VLAN
            ID="1">Untagged</VLAN>
        </interface>
      </nic>
      <nic>
        <nictype>port</nictype>
        <nicname>port4</nicname>
        <myid>
          <hostid>232</hostid>
          <nicid>239</nicid>
          <hostname>wbridge0</hostname>
          <nicname>port4</nicname>
        </myid>
        <nictype>port</nictype>
        <uniqueidentifier>239</uniqueidentifier>
        <usesdhcp>False</usesdhcp>
        <interface>
          <nicname>port4</nicname>
          <myip>
            <ip>0.0.0.0</ip>
            <mask>0.0.0.0</mask>
            <gateway>0.0.0.0</gateway>
            <type>ip</type>
          </myip>
          <VLAN
            ID="1">Untagged</VLAN>
        </interface>
      </nic>
      <nic>
        <nictype>port</nictype>
        <nicname>port5</nicname>
        <myid>
          <hostid>232</hostid>
          <nicid>240</nicid>
          <hostname>wbridge0</hostname>
          <nicname>port5</nicname>
        </myid>
        <nictype>port</nictype>
        <uniqueidentifier>240</uniqueidentifier>
        <usesdhcp>False</usesdhcp>
        <interface>
          <nicname>port5</nicname>
          <myip>
            <ip>0.0.0.0</ip>
            <mask>0.0.0.0</mask>
            <gateway>0.0.0.0</gateway>
            <type>ip</type>
          </myip>
          <VLAN
            ID="1">Untagged</VLAN>
        </interface>
      </nic>
    </device>
    <device>
      <hostname>wrepeater0</hostname>
      <size>100</size>
      <uniqueidentifier>276</uniqueidentifier>
      <location>260,420</location>
      <mytype>wrepeater</mytype>
      <isdns>False</isdns>
      <isdhcp>False</isdhcp>
      <gateway>
        <ip>192.168.2.1</ip>
        <mask>0.0.0.0</mask>
        <gateway>0.0.0.0</gateway>
        <type>gw</type>
      </gateway>
      <nic>
        <nictype>lo</nictype>
        <nicname>lo0</nicname>
        <myid>
          <hostid>276</hostid>
          <nicid>279</nicid>
          <hostname>wrepeater0</hostname>
          <nicname>lo0</nicname>
        </myid>
        <nictype>lo</nictype>
        <uniqueidentifier>279</uniqueidentifier>
        <usesdhcp>False</usesdhcp>
        <interface>
          <nicname>lo0</nicname>
          <myip>
            <ip>127.0.0.1</ip>
            <mask>255.0.0.0</mask>
            <gateway>0.0.0.0</gateway>
            <type>ip</type>
          </myip>
          <VLAN
            ID="1">Untagged</VLAN>
        </interface>
      </nic>
      <nic>
        <nictype>wlan</nictype>
        <nicname>wlan1</nicname>
        <myid>
          <hostid>276</hostid>
          <nicid>280</nicid>
          <hostname>wrepeater0</hostname>
          <nicname>wlan1</nicname>
        </myid>
        <nictype>wlan</nictype>
        <uniqueidentifier>280</uniqueidentifier>
        <usesdhcp>False</usesdhcp>
        <encryptionkey>myKey</encryptionkey>
        <ssid>my_SSID</ssid>
        <interface>
          <nicname>wlan1</nicname>
          <myip>
            <ip>192.168.2.10</ip>
            <mask>255.255.255.0</mask>
            <gateway>0.0.0.0</gateway>
            <type>ip</type>
          </myip>
          <VLAN
            ID="1">Untagged</VLAN>
        </interface>
      </nic>
      <nic>
        <nictype>wport</nictype>
        <nicname>wport2</nicname>
        <myid>
          <hostid>276</hostid>
          <nicid>281</nicid>
          <hostname>wrepeater0</hostname>
          <nicname>wport2</nicname>
        </myid>
        <nictype>wport</nictype>
        <uniqueidentifier>281</uniqueidentifier>
        <usesdhcp>False</usesdhcp>
        <encryptionkey>myKey</encryptionkey>
        <ssid>my_SSID</ssid>
        <interface>
          <nicname>wport2</nicname>
          <myip>
            <ip>0.0.0.0</ip>
            <mask>0.0.0.0</mask>
            <gateway>0.0.0.0</gateway>
            <type>ip</type>
          </myip>
          <VLAN
            ID="1">Untagged</VLAN>
        </interface>
      </nic>
    </device>
    <device>
      <hostname>wrouter1</hostname>
      <size>100</size>
      <uniqueidentifier>207</uniqueidentifier>
      <location>700,470</location>
      <mytype>wrouter</mytype>
      <isdns>False</isdns>
      <isdhcp>False</isdhcp>
      <gateway>
        <ip>192.168.6.1</ip>
        <mask>0.0.0.0</mask>
        <gateway>0.0.0.0</gateway>
        <type>gw</type>
      </gateway>
      <nic>
        <nictype>lo</nictype>
        <nicname>lo0</nicname>
        <myid>
          <hostid>207</hostid>
          <nicid>210</nicid>
          <hostname>wrouter1</hostname>
          <nicname>lo0</nicname>
        </myid>
        <nictype>lo</nictype>
        <uniqueidentifier>210</uniqueidentifier>
        <usesdhcp>False</usesdhcp>
        <encryptionkey />
        <ssid />
        <interface>
          <nicname>lo0</nicname>
          <myip>
            <ip>127.0.0.1</ip>
            <mask>255.0.0.0</mask>
            <gateway>0.0.0.0</gateway>
            <type>ip</type>
          </myip>
          <VLAN
            ID="1">Untagged</VLAN>
        </interface>
      </nic>
      <nic>
        <nictype>wan</nictype>
        <nicname>wan0</nicname>
        <myid>
          <hostid>207</hostid>
          <nicid>225</nicid>
          <hostname>wrouter1</hostname>
          <nicname>wan0</nicname>
        </myid>
        <nictype>wan</nictype>
        <uniqueidentifier>225</uniqueidentifier>
        <usesdhcp>False</usesdhcp>
        <encryptionkey />
        <ssid />
        <interface>
          <nicname>wan0</nicname>
          <myip>
            <ip>192.168.6.2</ip>
            <mask>255.255.255.0</mask>
            <gateway>0.0.0.0</gateway>
            <type>ip</type>
          </myip>
          <VLAN
            ID="1">Untagged</VLAN>
        </interface>
      </nic>
      <nic>
        <nictype>vpn</nictype>
        <nicname>vpn0</nicname>
        <myid>
          <hostid>207</hostid>
          <nicid>224</nicid>
          <hostname>wrouter1</hostname>
          <nicname>vpn0</nicname>
        </myid>
        <nictype>vpn</nictype>
        <uniqueidentifier>224</uniqueidentifier>
        <usesdhcp>False</usesdhcp>
        <encryptionkey>Test</encryptionkey>
        <ssid />
        <tunnelendpoint>
          <ip>192.168.5.2</ip>
          <mask>255.255.255.0</mask>
          <gateway>0.0.0.0</gateway>
          <type>ip_only</type>
        </tunnelendpoint>
        <interface>
          <nicname>vpn0</nicname>
          <myip>
            <ip>192.168.50.2</ip>
            <mask>255.255.255.0</mask>
            <gateway>0.0.0.0</gateway>
            <type>ip</type>
          </myip>
          <VLAN
            ID="1">Untagged</VLAN>
        </interface>
      </nic>
      <nic>
        <nictype>management_interface</nictype>
        <nicname>management_interface0</nicname>
        <myid>
          <hostid>207</hostid>
          <nicid>211</nicid>
          <hostname>wrouter1</hostname>
          <nicname>management_interface0</nicname>
        </myid>
        <nictype>management_interface</nictype>
        <uniqueidentifier>211</uniqueidentifier>
        <usesdhcp>False</usesdhcp>
        <encryptionkey />
        <ssid />
        <interface>
          <nicname>management_interface0</nicname>
          <myip>
            <ip>192.168.2.1</ip>
            <mask>255.255.255.0</mask>
            <gateway>0.0.0.0</gateway>
            <type>ip</type>
          </myip>
          <VLAN
            ID="1">Untagged</VLAN>
        </interface>
      </nic>
      <nic>
        <nictype>port</nictype>
        <nicname>port2</nicname>
        <myid>
          <hostid>207</hostid>
          <nicid>212</nicid>
          <hostname>wrouter1</hostname>
          <nicname>port2</nicname>
        </myid>
        <nictype>port</nictype>
        <uniqueidentifier>212</uniqueidentifier>
        <usesdhcp>False</usesdhcp>
        <encryptionkey />
        <ssid />
        <interface>
          <nicname>port2</nicname>
          <myip>
            <ip>0.0.0.0</ip>
            <mask>0.0.0.0</mask>
            <gateway>0.0.0.0</gateway>
            <type>ip</type>
          </myip>
          <VLAN
            ID="1">Untagged</VLAN>
        </interface>
      </nic>
      <nic>
        <nictype>port</nictype>
        <nicname>port3</nicname>
        <myid>
          <hostid>207</hostid>
          <nicid>213</nicid>
          <hostname>wrouter1</hostname>
          <nicname>port3</nicname>
        </myid>
        <nictype>port</nictype>
        <uniqueidentifier>213</uniqueidentifier>
        <usesdhcp>False</usesdhcp>
        <encryptionkey />
        <ssid />
        <interface>
          <nicname>port3</nicname>
          <myip>
            <ip>0.0.0.0</ip>
            <mask>0.0.0.0</mask>
            <gateway>0.0.0.0</gateway>
            <type>ip</type>
          </myip>
          <VLAN
            ID="1">Untagged</VLAN>
        </interface>
      </nic>
      <nic>
        <nictype>port</nictype>
        <nicname>port4</nicname>
        <myid>
          <hostid>207</hostid>
          <nicid>214</nicid>
          <hostname>wrouter1</hostname>
          <nicname>port4</nicname>
        </myid>
        <nictype>port</nictype>
        <uniqueidentifier>214</uniqueidentifier>
        <usesdhcp>False</usesdhcp>
        <encryptionkey />
        <ssid />
        <interface>
          <nicname>port4</nicname>
          <myip>
            <ip>0.0.0.0</ip>
            <mask>0.0.0.0</mask>
            <gateway>0.0.0.0</gateway>
            <type>ip</type>
          </myip>
          <VLAN
            ID="1">Untagged</VLAN>
        </interface>
      </nic>
      <nic>
        <nictype>port</nictype>
        <nicname>port5</nicname>
        <myid>
          <hostid>207</hostid>
          <nicid>215</nicid>
          <hostname>wrouter1</hostname>
          <nicname>port5</nicname>
        </myid>
        <nictype>port</nictype>
        <uniqueidentifier>215</uniqueidentifier>
        <usesdhcp>False</usesdhcp>
        <encryptionkey />
        <ssid />
        <interface>
          <nicname>port5</nicname>
          <myip>
            <ip>0.0.0.0</ip>
            <mask>0.0.0.0</mask>
            <gateway>0.0.0.0</gateway>
            <type>ip</type>
          </myip>
          <VLAN
            ID="1">Untagged</VLAN>
        </interface>
      </nic>
      <nic>
        <nictype>wport</nictype>
        <nicname>wport6</nicname>
        <myid>
          <hostid>207</hostid>
          <nicid>216</nicid>
          <hostname>wrouter1</hostname>
          <nicname>wport6</nicname>
        </myid>
        <nictype>wport</nictype>
        <uniqueidentifier>216</uniqueidentifier>
        <usesdhcp>False</usesdhcp>
        <encryptionkey>myKey</encryptionkey>
        <ssid>my_SSID</ssid>
        <interface>
          <nicname>wport6</nicname>
          <myip>
            <ip>0.0.0.0</ip>
            <mask>0.0.0.0</mask>
            <gateway>0.0.0.0</gateway>
            <type>ip</type>
          </myip>
          <VLAN
            ID="1">Untagged</VLAN>
        </interface>
      </nic>
      <nic>
        <nictype>wport</nictype>
        <nicname>wport7</nicname>
        <myid>
          <hostid>207</hostid>
          <nicid>217</nicid>
          <hostname>wrouter1</hostname>
          <nicname>wport7</nicname>
        </myid>
        <nictype>wport</nictype>
        <uniqueidentifier>217</uniqueidentifier>
        <usesdhcp>False</usesdhcp>
        <encryptionkey>myKey</encryptionkey>
        <ssid>my_SSID</ssid>
        <interface>
          <nicname>wport7</nicname>
          <myip>
            <ip>0.0.0.0</ip>
            <mask>0.0.0.0</mask>
            <gateway>0.0.0.0</gateway>
            <type>ip</type>
          </myip>
          <VLAN
            ID="1">Untagged</VLAN>
        </interface>
      </nic>
      <nic>
        <nictype>wport</nictype>
        <nicname>wport8</nicname>
        <myid>
          <hostid>207</hostid>
          <nicid>218</nicid>
          <hostname>wrouter1</hostname>
          <nicname>wport8</nicname>
        </myid>
        <nictype>wport</nictype>
        <uniqueidentifier>218</uniqueidentifier>
        <usesdhcp>False</usesdhcp>
        <encryptionkey>myKey</encryptionkey>
        <ssid>my_SSID</ssid>
        <interface>
          <nicname>wport8</nicname>
          <myip>
            <ip>0.0.0.0</ip>
            <mask>0.0.0.0</mask>
            <gateway>0.0.0.0</gateway>
            <type>ip</type>
          </myip>
          <VLAN
            ID="1">Untagged</VLAN>
        </interface>
      </nic>
      <nic>
        <nictype>wport</nictype>
        <nicname>wport9</nicname>
        <myid>
          <hostid>207</hostid>
          <nicid>219</nicid>
          <hostname>wrouter1</hostname>
          <nicname>wport9</nicname>
        </myid>
        <nictype>wport</nictype>
        <uniqueidentifier>219</uniqueidentifier>
        <usesdhcp>False</usesdhcp>
        <encryptionkey>myKey</encryptionkey>
        <ssid>my_SSID</ssid>
        <interface>
          <nicname>wport9</nicname>
          <myip>
            <ip>0.0.0.0</ip>
            <mask>0.0.0.0</mask>
            <gateway>0.0.0.0</gateway>
            <type>ip</type>
          </myip>
          <VLAN
            ID="1">Untagged</VLAN>
        </interface>
      </nic>
      <nic>
        <nictype>wport</nictype>
        <nicname>wport10</nicname>
        <myid>
          <hostid>207</hostid>
          <nicid>220</nicid>
          <hostname>wrouter1</hostname>
          <nicname>wport10</nicname>
        </myid>
        <nictype>wport</nictype>
        <uniqueidentifier>220</uniqueidentifier>
        <usesdhcp>False</usesdhcp>
        <encryptionkey>myKey</encryptionkey>
        <ssid>my_SSID</ssid>
        <interface>
          <nicname>wport10</nicname>
          <myip>
            <ip>0.0.0.0</ip>
            <mask>0.0.0.0</mask>
            <gateway>0.0.0.0</gateway>
            <type>ip</type>
          </myip>
          <VLAN
            ID="1">Untagged</VLAN>
        </interface>
      </nic>
      <nic>
        <nictype>wport</nictype>
        <nicname>wport11</nicname>
        <myid>
          <hostid>207</hostid>
          <nicid>221</nicid>
          <hostname>wrouter1</hostname>
          <nicname>wport11</nicname>
        </myid>
        <nictype>wport</nictype>
        <uniqueidentifier>221</uniqueidentifier>
        <usesdhcp>False</usesdhcp>
        <encryptionkey>myKey</encryptionkey>
        <ssid>my_SSID</ssid>
        <interface>
          <nicname>wport11</nicname>
          <myip>
            <ip>0.0.0.0</ip>
            <mask>0.0.0.0</mask>
            <gateway>0.0.0.0</gateway>
            <type>ip</type>
          </myip>
          <VLAN
            ID="1">Untagged</VLAN>
        </interface>
      </nic>
      <nic>
        <nictype>wport</nictype>
        <nicname>wport12</nicname>
        <myid>
          <hostid>207</hostid>
          <nicid>222</nicid>
          <hostname>wrouter1</hostname>
          <nicname>wport12</nicname>
        </myid>
        <nictype>wport</nictype>
        <uniqueidentifier>222</uniqueidentifier>
        <usesdhcp>False</usesdhcp>
        <encryptionkey>myKey</encryptionkey>
        <ssid>my_SSID</ssid>
        <interface>
          <nicname>wport12</nicname>
          <myip>
            <ip>0.0.0.0</ip>
            <mask>0.0.0.0</mask>
            <gateway>0.0.0.0</gateway>
            <type>ip</type>
          </myip>
          <VLAN
            ID="1">Untagged</VLAN>
        </interface>
      </nic>
      <nic>
        <nictype>wport</nictype>
        <nicname>wport13</nicname>
        <myid>
          <hostid>207</hostid>
          <nicid>223</nicid>
          <hostname>wrouter1</hostname>
          <nicname>wport13</nicname>
        </myid>
        <nictype>wport</nictype>
        <uniqueidentifier>223</uniqueidentifier>
        <usesdhcp>False</usesdhcp>
        <encryptionkey>myKey</encryptionkey>
        <ssid>my_SSID</ssid>
        <interface>
          <nicname>wport13</nicname>
          <myip>
            <ip>0.0.0.0</ip>
            <mask>0.0.0.0</mask>
            <gateway>0.0.0.0</gateway>
            <type>ip</type>
          </myip>
          <VLAN
            ID="1">Untagged</VLAN>
        </interface>
      </nic>
      <route>
        <ip>192.168.1.0</ip>
        <mask>255.255.255.0</mask>
        <gateway>192.168.50.1</gateway>
        <type>route</type>
      </route>
    </device>
    <device>
      <hostname>microwave0</hostname>
      <size>100</size>
      <uniqueidentifier>309</uniqueidentifier>
      <location>320,350</location>
      <mytype>microwave</mytype>
      <isdns>False</isdns>
      <isdhcp>False</isdhcp>
      <gateway>
        <ip>0.0.0.0</ip>
        <mask>0.0.0.0</mask>
        <gateway>0.0.0.0</gateway>
        <type>gw</type>
      </gateway>
      <nic>
        <nictype>lo</nictype>
        <nicname>lo0</nicname>
        <myid>
          <hostid>309</hostid>
          <nicid>310</nicid>
          <hostname>microwave0</hostname>
          <nicname>lo0</nicname>
        </myid>
        <nictype>lo</nictype>
        <uniqueidentifier>310</uniqueidentifier>
        <usesdhcp>False</usesdhcp>
        <encryptionkey />
        <ssid />
        <interface>
          <nicname>lo0</nicname>
          <myip>
            <ip>127.0.0.1</ip>
            <mask>255.0.0.0</mask>
            <gateway>0.0.0.0</gateway>
            <type>ip</type>
          </myip>
          <VLAN
            ID="1">Untagged</VLAN>
        </interface>
      </nic>
      <nic>
        <nictype>eth</nictype>
        <nicname>eth0</nicname>
        <myid>
          <hostid>309</hostid>
          <nicid>311</nicid>
          <hostname>microwave0</hostname>
          <nicname>eth0</nicname>
        </myid>
        <nictype>eth</nictype>
        <uniqueidentifier>311</uniqueidentifier>
        <usesdhcp>False</usesdhcp>
        <encryptionkey />
        <ssid />
        <interface>
          <nicname>eth0</nicname>
          <myip>
            <ip>0.0.0.0</ip>
            <mask>0.0.0.0</mask>
            <gateway>0.0.0.0</gateway>
            <type>ip</type>
          </myip>
          <VLAN
            ID="1">Untagged</VLAN>
        </interface>
      </nic>
    </device>
    <link>
      <SrcNic>
        <hostid>124</hostid>
        <nicid>129</nicid>
        <hostname>net_switch1</hostname>
        <nicname>port3</nicname>
      </SrcNic>
      <DstNic>
        <hostid>207</hostid>
        <nicid>212</nicid>
        <hostname>wrouter1</hostname>
        <nicname>port2</nicname>
      </DstNic>
      <hostname>net_switch1_link_wrouter1</hostname>
      <linktype>normal</linktype>
      <uniqueidentifier>226</uniqueidentifier>
    </link>
    <link>
      <SrcNic>
        <hostid>137</hostid>
        <nicid>139</nicid>
        <hostname>pc1</hostname>
        <nicname>eth0</nicname>
      </SrcNic>
      <DstNic>
        <hostid>124</hostid>
        <nicid>127</nicid>
        <hostname>net_switch1</hostname>
        <nicname>port1</nicname>
      </DstNic>
      <hostname>pc1_link_net_switch1</hostname>
      <linktype>normal</linktype>
      <uniqueidentifier>149</uniqueidentifier>
    </link>
    <link>
      <SrcNic>
        <hostid>143</hostid>
        <nicid>145</nicid>
        <hostname>laptop1</hostname>
        <nicname>eth0</nicname>
      </SrcNic>
      <DstNic>
        <hostid>124</hostid>
        <nicid>128</nicid>
        <hostname>net_switch1</hostname>
        <nicname>port2</nicname>
      </DstNic>
      <hostname>laptop1_link_net_switch1</hostname>
      <linktype>normal</linktype>
      <uniqueidentifier>150</uniqueidentifier>
    </link>
    <link>
      <SrcNic>
        <hostid>243</hostid>
        <nicid>245</nicid>
        <hostname>pc3</hostname>
        <nicname>eth0</nicname>
      </SrcNic>
      <DstNic>
        <hostid>232</hostid>
        <nicid>237</nicid>
        <hostname>wbridge0</hostname>
        <nicname>port2</nicname>
      </DstNic>
      <hostname>pc3_link_wbridge0</hostname>
      <linktype>normal</linktype>
      <uniqueidentifier>246</uniqueidentifier>
    </link>
    <link>
      <SrcNic>
        <hostid>232</hostid>
        <nicid>238</nicid>
        <hostname>wbridge0</hostname>
        <nicname>port3</nicname>
      </SrcNic>
      <DstNic>
        <hostid>256</hostid>
        <nicid>258</nicid>
        <hostname>printer0</hostname>
        <nicname>eth0</nicname>
      </DstNic>
      <hostname>wbridge0_link_printer0</hostname>
      <linktype>normal</linktype>
      <uniqueidentifier>259</uniqueidentifier>
    </link>
    <link>
      <SrcNic>
        <hostid>232</hostid>
        <nicid>236</nicid>
        <hostname>wbridge0</hostname>
        <nicname>wlan1</nicname>
      </SrcNic>
      <DstNic>
        <hostid>276</hostid>
        <nicid>281</nicid>
        <hostname>wrepeater0</hostname>
        <nicname>wport2</nicname>
      </DstNic>
      <hostname />
      <linktype>wireless</linktype>
      <uniqueidentifier>338</uniqueidentifier>
    </link>
    <link>
      <SrcNic>
        <hostid>276</hostid>
        <nicid>280</nicid>
        <hostname>wrepeater0</hostname>
        <nicname>wlan1</nicname>
      </SrcNic>
      <DstNic>
        <hostid>207</hostid>
        <nicid>216</nicid>
        <hostname>wrouter1</hostname>
        <nicname>wport6</nicname>
      </DstNic>
      <hostname />
      <linktype>wireless</linktype>
      <uniqueidentifier>339</uniqueidentifier>
    </link>
    <nettest>
      <shost>pc1</shost>
      <dhost>printer0</dhost>
      <thetest>SuccessfullyPings</thetest>
    </nettest>
    <nettest>
      <shost>pc1</shost>
      <dhost>pc3</dhost>
      <thetest>SuccessfullyPings</thetest>
    </nettest>
    <nettest>
      <shost>microwave0</shost>
      <dhost>All</dhost>
      <thetest>LockAll</thetest>
    </nettest>
    <nettest>
      <shost>wbridge0</shost>
      <dhost>--</dhost>
      <thetest>LockLocation</thetest>
    </nettest>
    <nettest>
      <shost>wrepeater0</shost>
      <dhost>--</dhost>
      <thetest>LockLocation</thetest>
    </nettest>
    <nettest>
      <shost>wrouter1</shost>
      <dhost>--</dhost>
      <thetest>LockLocation</thetest>
    </nettest>
    <VLANName
      ID="1"
      Color="Blue">Default</VLANName>
  </Network>
</EduNetworkBuilder>